[Contents] [Prev] [Next] [Report an Error]

# cOC3/STM1 Single-Mode Intermediate Reach Module Combination

> Line module label | cOCx/STMx F0
> I/O module label | cOC3 STM1 F0 I/O SINGLE MODE
> Number of I/O ports | 4
> Software release | First supported: 2.2.0 Final supported: Not applicable
> Description | 130 W OC3/STM1 channelized to DS3, DS1, E1, and DS0
> Type | EFA ASIC
> Capability | OC3/STM1 DS3, DS1 T1, E1 DS0 HDLC framing
> Software features | See Channelized OCx/STMx Modules for information about the layer 2 and layer 3 protocols and applications that this module combination supports.
> Model compatibility | ERX7xx models ERX14xx models ERX310 router
> SRP module compatibility | SRP-5G+ SRP-10G SRP-40G SRP-40G PLUS SRP-SE10G
> Module redundancy support | 1:N redundancy NOTE: Line module redundancy is not supported on the ERX310 router.
> Cables and connectors | Up to four SC full duplex connectors Tx power: min: –15 dBm max: –8 dBm Center wavelength: 1310 nm Rx input power: min: –31 dBm max: –8 dBm Rated for 15 km (9.3 miles) of 9-micron core cable See ERX Hardware Guide, Chapter 5, Cabling ERX Routers for more information.
> LEDs | See Module LEDs.
> Alarms, errors, and events | See Monitoring Interfaces in JUNOSe Physical Layer Configuration Guide, Chapter 4, Configuring Channelized OCx/STMx Interfaces.

[Contents] [Prev] [Next] [Report an Error]