[Contents] [Prev] [Next] [Report an Error]

# Unchannelized T3 Modules

Table 20: Unchannelized T3 Modules

Protocol or Application | COCX-F3 Line Modules with CT3/T3 12 I/O Modules | OCx/STMx ATM Line Modules with 4xDS3 ATM I/O Modules | CT3/T3-F0 Line Modules with CT3/T3 12 I/O Modules
--- | --- | --- | ---
Accepts traffic destined for GRE tunnels or DVMRP (IP-in-IP) tunnels | Yes | Yes | Yes
APS/MSP | No | No | No
ATM (point-to-point) | No | Yes | No
BERT | Yes | No | Yes
BFD | No | No | No
BGP | Yes | Yes | Yes
BGP/MPLS VPNs | Yes | Yes | Yes
Bridged Ethernet | No | Yes | No
Bridged IP | No | Yes | No
Cisco HDLC | Yes | No | Yes
DHCP external server | No | Yes | No
DHCP local server | No | Yes | No
DVMRP and GRE support—access side | Yes | Yes | Yes
DVMRP and GRE support—access side | No | No | No
Dynamic interfaces | No | Yes | No
F4 OAM and F5 OAM (ATM administration) | No | Yes | No
FDL (facilities data link) | No | No | No
Firewall | Yes | Yes | Yes
Frame Relay | Yes | No | Yes
ICR | No | No | No
IEEE 802.3ad link aggregation | No | No | No
IP | Yes | Yes | Yes
IP multicast | No | No | No
IP reassembly for tunneled packets | No | No | No
IPSec | No | No | No
IPv6 | No | No | No
IPv6 multicast | Yes | Yes | Yes
IPv6 neighbor discovery | No | No | No
IS-IS | Yes | Yes | Yes
J-Flow Statistics | Yes | Yes | Yes
L2TP/IPSec | No | No | No
LAC support—access side | No | Yes | No
LAC support—peer side | No | Yes | No
LNS support—peer side | No | Yes | No
Local loopback | Yes | No | Yes
MDL (maintenance data link) | Yes | No | Yes
Mobile IP home agent | No | No | No
MPLS | Yes (over PPP and Cisco HDLC; also supports Martini encapsulation of HDLC and Frame Relay over MPLS) | Yes | Yes (over PPP and Cisco HDLC; also supports Martini encapsulation of HDLC and Frame Relay over MPLS)
Multilink Frame Relay | Yes | No | Yes
Multilink PPP | Yes (with fragmentation and reassembly) | No | Yes
Network Address Translation (NAT) | Yes | Yes | Yes
NBMA (multipoint ATM) | No | Yes | No
OSPF | Yes | Yes | Yes
Packet Mirroring | Yes | Yes | Yes
Packet over SONET | No | No | No
PPP | Yes | Yes | Yes
PPPoE | No | Yes | No
Remote loopback | Yes | No | Yes
RIP | Yes | Yes | Yes
Subscriber interfaces (static) | Yes | Yes (over bridged Ethernet and IPoA) | Yes
Subscriber interfaces (dynamic) | Yes | Yes (over bridged Ethernet) | Yes
Transparent bridging | No | Yes | No
Tunnel-server ports | No | No | No
Unified ISSU | No | Yes | No
VPLS (network interfaces) | No | Yes | No
VPLS (virtual core interfaces) | Yes | Yes | Yes
VRRP | No | No | No

[Contents] [Prev] [Next] [Report an Error]