> - Downloads
> - radius connect-info-format

> # radius connect-info-format

> #### Syntax

> radius connect-info-format { l2tp-connect-speed |
> l2tp-connect-speed-rx-when-equal }

> no radius connect-info-format

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Specifies the format of RADIUS attribute 77, Connect-Info, on the LNS. The format uses the received L2TP connect-speed AVPs that the LAC sends to the LNS. The no version restores the default, in which the LNS does not generate the Connect-Info attribute.

> #### Options

> - l2tp-connect-speed—Specifies that the Connect-Info attribute include only the RX speed when the RX speed is different from the TX speed and is greater than zero.
> - l2tp-connect-speed-rx-when-equal—Specifies that the Connect-Info attribute always include the RX speed when the speed is greater than zero.

> #### Mode

> Global Configuration

> #### Published: 2009-10-08

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.