[Contents] [Prev] [Next] [Index] [Report an Error]

## Index

Symbols A B C D E F G H I K L M N O P R S T U V W

Symbols

> 802.3ad switch 1

A

> access lists, BGP 1
>   assigning weights to neighbors 1
>   distributing neighbor information 1
> access-list command 1, 2
> address families 1
>   L2VPN 1, 2, 3, 4, 5, 6
>   multicast IPv4 1, 2, 3
>   multicast IPv6 1, 2, 3
>   route-target 1, 2
>   unicast IPv4 1, 2, 3
>   unicast IPv6 1, 2, 3
>   VPLS 1, 2, 3, 4, 5
>   VPN-IPv4 1, 2, 3
>   VPN-IPv6 1, 2, 3
>   VPWS 1, 2, 3, 4, 5
> address-family command 1, 2, 3, 4, 5
>   for L2VPN address family 1
>   for VPWS address family 1
> administrative distance
>   BGP, setting 1
> admission control, MPLS 1
> advertise-map keyword (aggregate-address) 1
> aggregate addresses
>   BGP 1
> aggregate-address command 1
> aggregation, LDP FEC 1
> aggregator, BGP 1
> append-after command 1
> APS/MSP (Automatic Protect Switching/Multiplex Section Protection) 1
> areas, OSPF
>   defining 1
> AS (autonomous system) 1
>   advertising networks in 1
>   confederation 1
>   IGP (interior gateway protocol) 1
>   managing a large-scale 1
> AS path filtering 1
> AS-path, BGP
>   access lists, modifying 1
>   attribute 1
>   filtering 1
> as-set keyword (aggregate-address) 1
> ATM (Asynchronous Transfer Mode)
>   AAL0 encapsulation 1
>   AAL5 encapsulation 1
>   Martini encapsulation 1
>   over MPLS 1
>   passthrough for ATM over MPLS 1, 2
>   VCC cell relay encapsulation
>     configuring 1
>     overview 1
> ATM cells
>   concatenation of multiple
>     for transportation over a single pseudowire 1
>   transported over a single pseudowire, subset of
>     discarded on he remote PE device 1
> atm commands
>   atm cell-packing 1
>   atm mcpt-timers 1
>   atm pvc 1, 2
> ATM line modules
>   and transport of a subset of ATM VCs
>     over a single pseudowire 1
>   hardware limitations
>     and support of multiple VCs over a pseudowire 1
> ATM Martini cell packing timer
>   expired time interval
>     and forwarding of MPLs packets 1
>   for concatenation of multiple cells
>     and transmission over a single pseudowire 1
> ATM n-to-one VCC cell transport (0x0009) pseudowire (PW) type
>   used by LDP
>     for subset of ATM VCs over a pseudowire transport 1
> ATM ports
>   changed to LOS state
>     and multiple VCs over a single pseudowire 1
>   configuring cell concatenation parameters
>     requirements 1
>   connectivity between two of them
>     emulated using multiple VCs transport over a pseudowire 1
>   not changed to LOS state
>     during a failure on the pseudowire 1
> ATM virtual circuits
>     1
>   adding MPLS Martini circuit configuration
>     for multiple VCs transport over a pseudowire 1
>   and emulation of connectivity
>     between ATM ports 1
>   based on RFC 4816
>     exception with subset of ATM cells transport 1
>   concatenation of multiple cells
>     requirements for configuring 1
>   configuring a subset of
>     using the mpls-relay atm vpi-range command 1
>   configuring VPI/VCI ranges
>     1
>   hardware limitations of ATM LMs
>     and transport of multiple VCs over a pseudowire 1
>   in Martini topologies
>     transportation over a single pseudowire 1
>   received on an ATM port
>     opening VCs on the SAR scheduler 1
>   transmission of a subset of ATM cells over a pseudowire
>     deployment scenario 1
>   transmission of multiple cells over a pseudowire
>     high availability and 1
>     limit on total number of 1
>     performance impact 1
>     unified ISSU and 1
>     verifying cell concatenation 1
>     verifying VCI/VPI ranges 1
>   transmission of multiple VCs over a single pseudowire
>     interoperation with cell relay on a subinterface 1
>   transport of multiple cells over a pseudowire
>     and ATM n-to-one VCC cell transport (0x0009) pseudowire (PW) type 1
>   transportation of cells from multiple circuits
>     over a single pseudowire 1
>   transportation of multiple ATM cells
>     concatetation 1
> atomic-aggregate, BGP 1
> attribute-map keyword (aggregate-address) 1
> authentication
>   BGP 1
>   MPLS
>     LDP MD5 1
>     RSVP-TE 1
> auto-summary command 1
> autoconfiguration, LDP 1
> autonomous system. See AS

B

> backdoor link, OSPF 1
> backdoor route, BGP 1
> backup tunnels, MPLS RSVP-TE 1
> bandwidth command 1
> baseline commands
>   baseline bridge 1
>   baseline bridge interface 1
>   baseline bridge interface vpls 1
>   baseline ip bgp 1
>   baseline mpls interface 1, 2
>   baseline mpls label 1
>   baseline mpls next-hop 1, 2
> BFD (Bidirectional Forwarding Detection)
>   BGP peer reachability detection 1
>   RSVP-TE, configuring for 1
> BGP (Border Gateway Protocol) 1
>   access lists 1
>   administrative distance 1
>   administrative shutdown 1, 2
>   advertising networks in ASs 1
>   advertising routes conditionally 1
>   advertising two best routes 1
>   aggregator path attribute 1
>   AS-path attribute 1
>   atomic-aggregate path attribute 1
>   authentication on TCP connection 1
>   automatic fallover 1
>   automatic summarization of routes 1
>   backdoor routes 1
>   BFD 1
>     and graceful restart 1
>     packet rates 1
>     session events 1
>   BGP/MPLS VPNs 1
>     configuring sessions for 1
>   capabilities 1
>   capability negotiation 1
>   changing BGP policies 1
>   checking AS number from external peer 1
>   Cisco-proprietary route refresh capability 1
>   community lists 1
>   community path attribute 1
>   conditional advertising 1
>   configuration inheritance 1
>   configuring 1
>     default routes 1
>     peer groups 1
>     route reflectors 1
>     routing policy 1
>   cooperative route filtering capability 1
>   default next-hop address 1
>   deleting BGP sessions 1, 2
>   deprecated dynamic capability negotiation capability 1, 2
>   displaying CIDR routes 1
>   dynamic capability negotiation capability 1, 2
>   dynamic peering 1
>   EBGP 1
>   ECMP 1, 2
>   enable BGP routing 1
>   enable routing 1
>   enable routing for BGP/MPLS VPNs 1, 2
>   End-of-RIB marker 1
>   extended community path attribute 1
>   features 1
>   four-octet AS numbers capability 1
>   graceful restart 1, 2
>     and BFD 1
>   IBGP 1
>   inheritance of configuration values 1
>   keepalive message 1
>   keepalives and BFD 1
>   L2VPNs, configuring 1
>   lenient behavior for error recovery 1
>   link-local next hops 1
>   local-pref path attribute 1
>   messages 1
>   monitoring 1
>   multiexit discriminator path attribute 1
>   multiprotocol extensions 1
>   multiprotocol extensions capability 1
>   neighbors and peer groups, shutting down 1
>   next-hop path attribute 1
>   notification message 1
>   open message 1
>   originator-ID path attribute 1
>   passive peers 1
>   path 1
>   path attribute 1
>   path selection process 1
>   peer (neighbor) 1
>   peer groups 1
>   peer type, set the 1
>   platform considerations 1
>   policies, soft reconfiguration of 1
>   promiscuous peers 1
>   reapplying BGP policies 1
>   redistributing BGP routes 1
>   reduce the number of meshed peers 1
>   remove BGP dynamic peers 1
>   resetting BGP sessions 1, 2
>   route refresh capability 1
>   route-refresh message 1
>   routes, using for other protocols 1
>   running out of memory 1
>   sessions 1
>     assigning interface to 1
>     automatic restoration of 1
>     deleting BGP 1, 2
>     hard clearing 1
>     resetting and clearing 1
>     route 1
>     soft clearing 1
>   shutting BGP down when low on memory 1
>   speaker 1
>   synchronization 1
>   troubleshooting 1
>   update message 1
>   VPLS, configuring 1
> bgp commands 1
>   bgp advertise-best-external-to-internal 1
>   bgp advertise-inactive 1
>   bgp always-compare-med 1, 2
>   bgp bestpath med confed 1
>   bgp client-to-client reflection 1
>   bgp cluster-id 1
>   bgp confederation identifier 1
>   bgp confederation peers 1, 2
>   bgp dampening 1
>   bgp default ipv4-unicast 1
>   bgp default local-preference 1, 2
>   bgp default route-target filter 1
>   bgp enforce-first-as 1
>   bgp fast-external-fallover 1
>   bgp log-neighbor-changes 1
>   bgp redistribute-internal 1
>   bgp shutdown 1
>   bgp wait-on-end-of-rib 1
>   See also show bgp ipv6 commands
> bgp graceful-restart commands
>   bgp graceful-restart 1
>   bgp graceful-restart restart-time 1
>   bgp graceful-restart stalepaths-time 1
>   bgp graceful-restartpath-selection-defer-time-limit 1
> BGP-based VPLS See VPLS (virtual private LAN service)
> BGP/MPLS VPNs
>   address family, disabling default 1
>   advertisement rules with route-target filtering 1
>   applications 1
>   AS number
>     advertising prefixes with duplicate 1
>     using for all CE sites 1
>   BGP advertising rules for routes 1
>   BGP sessions, configuring 1
>   customer edge device 1
>   data transport 1
>   default route to shared interface 1
>   ECMP 1, 2
>   ECMP indirect next hops 1
>   export list 1
>   export map, setting the 1
>   extended community, route target 1
>   fallback global 1
>   fallback global example 1, 2
>   fast reconvergence 1
>   filtering routes 1
>   full mesh VPN 1
>   global export map
>     example 1
>     IPv6 VPN routes 1
>     setting the 1
>   global import map to import specific routes 1
>   hub-and-spoke VPN 1
>   IGP routes, advertising 1
>   IGPs, configuring on VRF 1
>   import list 1
>   import map, setting the 1
>   inter-AS (interprovider) services
>     IPv4 1
>     IPv6 1
>   interaction with OSPF 1
>   intra-AS services
>     IPv4 1
>     IPv6 1
>   IPv6 over IPv4 1, 2
>   L2VPNs and 1
>   L2VPNs, configuring 1
>   label-switching routers 1, 2
>   labeled and unlabeled routes, sending 1
>   labeled unicast routes, processing 1
>   labeled VPN routes, processing 1
>   maximum number of external best paths for route target filtering 1
>   maximum routes 1
>   monitoring 1
>   MP-Reach-NLRI attribute 1
>   MP-Unreach-NLRI attribute 1
>   MPLS labels 1
>   next hops, check reachability 1
>   OSPF backdoor link 1, 2
>   OSPF configuration 1
>   OSPF domain identifier attribute 1
>   OSPF route type attribute 1
>   OSPF routes
>     distributing between PEs 1
>     distributing from CE to PE 1
>     distributing from PE to CE 1
>   OSPF routing information, preserving 1
>   OSPF routing loops, preventing 1
>   overriding AS number for CE sites 1
>   parent VR, peering with VRF 1
>   path failure, ECMP 1
>   peering between VRF and parent VR 1
>   platform considerations 1
>   provider core routers 1
>   provider edge routers 1
>   providing Internet access 1
>   pruning failed ECMP paths 1
>   reachability of next hops 1
>   route distinguisher 1
>   route processing by BGP 1
>   route reachability information 1
>   route target
>     configuring VPN topologies 1
>     defining 1
>   route-target extended community 1
>   route-target filtering 1
>   route-target filtering, disabling 1
>   route-target membership attribute 1
>   routing loops, preventing 1
>   RT-MEM-NLRI attribute 1
>   RT-MEM-NLRI routing updates 1
>   secondary routing table lookup 1
>   setting maximum route limits 1
>   sham link, OSPF 1
>   site-of-origin to prevent routing loops 1
>   static routes to shared IP interface 1
>   static routes, advertising 1
>   traffic flow from Internet to VPN 1
>   traffic flow from VPN to Internet 1
>   transporting packets 1
>   troubleshooting 1, 2
>   unlabeled unicast routes, processing 1
>   update message enhancement 1
>   VPLS 1
>   VPLS, configuring 1
>   VPN services, configuring 1
>   VPN topologies, configuring with route targets 1
>     full-mesh 1
>     hub-and-spoke 1
>     overlapping 1
>   VPN-IPv4 address 1
>   VPNs between ASs
>     IPv4 1
>     IPv6 1
>   VPNs within an AS
>     IPv4 1
>     IPv6 1
>   VRF 1
> Bidirectional Forwarding Detection. See BFD
> Border Gateway Protocol. See BGP
> bridge commands 1
>   bridge acquire 1
>   bridge address 1
>   bridge aging-time 1
>   bridge learn 1
>   bridge snmp-trap link-status 1
>   bridge vpls rd 1
>   bridge vpls route-target 1
>   bridge vpls site-name site-id 1
>   bridge vpls site-range 1
>   bridge vpls transport-virtual-router 1, 2
>   bridge-group 1
>   See also show bridge commands
> bridging, transparent
>   and VPLS 1
> bundle messages, MPLS 1
> bypass tunnels, MPLS RSVP-TE 1

C

> candidate ports 1
> capabilities, BGP
>   Cisco-proprietary route refresh 1, 2
>   cooperative route filtering 1, 2
>   deprecated dynamic capability negotiation 1
>   dynamic capability negotiation 1, 2
>   four-octet AS numbers 1, 2
>   graceful restart 1, 2
>   multiprotocol extensions 1
>   route refresh 1, 2
> capability codes 1
> capability negotiation, BGP 1
> carrier-of-carriers IPv4 VPNs 1
>   enabling 1
> carrier-of-carriers IPv6 VPNs 1
> CE (customer edge device) 1, 2
> CE-side load balancing 1
> cell aggregation See concatenation
> cell relay encapsulation
>   for a single VC and multiple VCs
>     pseudowire type used 1
> cell relay encapsulation, VCC. See VCC cell relay encapsulation
> check-vpn-next-hops command 1
> CIDR (Classless Interdomain Routing)
>   configuring addresses 1
>   displaying BGP routes 1
> cleanout-timeout-factor command 1, 2
> clear
>   BGP hard 1
>   BGP soft 1
> clear bgp ipv6 commands
>   clear bgp ipv6 1
>   clear bgp ipv6 dampening 1
>   clear bgp ipv6 dynamic-peers 1
>   clear bgp ipv6 redistribution 1
> clear BGP sessions 1
> clear bridge commands
>   clear bridge 1
>   clear bridge address 1
>   clear bridge interface 1
>   clear bridge interface vpls 1
> clear commands
>   clear access-list 1
>   clear ip bgp wait-end-of-rib 1
>   clear ip routes 1
>   clear rsvp authentication 1
> clear ip bgp commands
>   clear ip bgp 1, 2, 3
>   clear ip bgp dampening 1, 2, 3, 4
>   clear ip bgp dynamic-peers 1
>   clear ip bgp redistribution 1
>   clear ip bgp soft prefix-filter 1
>   clear ip bgp wait-end-of-rib 1, 2
> clear ip commands
>   clear ip tunnel-routes 1, 2
> clear mpls commands
>   clear mpls dynamic-interfaces on-major-interfaces 1
>   clear mpls ldp 1
> codes, BGP capability 1
> communities, BGP
>   attributes 1
>   extended 1
> community lists, BGP 1, 2
> concatenation
>   of multiple ATM cells
>     for transmission over a single MPLS packet 1
>     maximum number 1
>     not using LDP signalling method 1
>     using a timer specified interval 1
> confederations 1
> configuration example
>   for multiple ATM virtual circuits transport
>     over a single pseudowire 1
> connectivity, verify and troubleshoot MPLS 1
> conventions
>   notice icons 1
>   text and syntax 1
> cooperative route filtering capability 1
> core non-VPN RIB 1, 2
> core VPN RIB 1, 2
> cross-connects, local 1, 2, 3, 4
> customer edge (CE) device 1
> customer support 1
>   contacting JTAC 1

D

> data path failure
>   detecting RSVP-TE 1
> deaggregation, LDP FEC 1
> debug commands
>   debug ip bgp 1
>   debug ip mbgp 1
>   undebug ip bgp 1
>   undebug ip mbgp 1
> default routes
>   BGP routing 1
> default-fields commands
>   default-fields peer 1
>   default-fields route 1
> default-information originate command 1, 2
> detecting RIP data path failure 1
> disable-dynamic-redistribute command 1
> discovery, LDP
>   basic 1
>   extended 1
> distance bgp command 1, 2
> documentation set
>   comments on 1
> domain, VPLS 1
> domain-id command 1
> domain-tag command 1
> dont-install-routes command 1
> DS-BGP routers 1
> dual-stack BGP routers 1
> dynamic capability negotiation 1
> dynamic interfaces, created by MPLS 1
> dynamic peering, BGP 1
> dynamic peers, remove BGP 1
> dynamic route redistribution, disabling in BGP 1
> dynamically learned defaults 1

E

> E-LSP 1, 2
> EBGP (external Border Gateway Protocol)
>   updates in indirectly connected networks 1
> echo reply packets, MPLS 1
> echo request packets, MPLS 1
> ECMP (equal-cost multipath)
>   BGP 1
>   BGP/MPLS VPNs 1, 2
>   MPLS indirect next hops 1
>   path failures in BGP/MPLS VPNs 1
>   pruning failed paths 1
> enable a protocol
>   BGP routing 1, 2, 3
> enable protocols
>   BGP routing 1
> encapsulations
>   ATM AAL0 1
>   ATM AAL05 1
> equal-cost multipath support on MPLS 1
> Ethernet aggregation and Martini layer 2 transport 1
> Ethernet raw mode encapsulation
>   overview 1
> Ethernet/VLAN over MPLS (Multiprotocol Label Switching)
>   configuration steps 1
>   overview 1
> exit-address-family command 1, 2, 3, 4, 5, 6
> explicit null label, advertise the 1
> export map
>   setting the BGP/MPLS VPN 1
>   use 1
> export map command 1
> extended communities
>   BGP 1, 2
>   route target 1
> external administrative distance, BGP 1
> external BGP
>   EBGP 1
> external-paths command 1

F

> F4 OAM cells
>   not carried on the same pseudowire as data cells
>     unopened OAM circuits 1
> F5 Operations Administration and Maintenance (OAM) cells
>   and transmission of data cells over the same pseudowire
>     same VCI/VPI values as the data cells 1
> fast reroute extension, MPLS 1
> FEC aggregation, LDP 1
> FEC deaggregation, LDP 1
> filter BGP/MPLS VPN routes 1
> filter lists, BGP 1, 2
> four-octet AS number capability 1
> Frame Relay
>   over MPLS 1
>     configuration example 1
> full-mesh VPNs, configure with route targets 1

G

> global export map
>   and IPv6 1
>   setting the BGP/MPLS VPN 1
>   use 1
> global export map command 1
> global import map
>   use 1
> global import map command 1
> global import map to import specific routes 1
> graceful restart
>   configuring RSVP-TE 1
>   LDP 1
>   RSVP-TE 1
> graceful restart capability 1

H

> hard clear of BGP sessions 1
> hardware limitations
>   with ATM line modules
>     and support of multiple VCs over a single pseudowire 1
> HDLC (High-Speed Data Link Control) layer 2 services over MPLS
>   configuring 1
>   overview 1
> hello commands
>   hello hold-time 1, 2
>   hello interval 1, 2
> hello messages
>   LDP link 1
>   LDP targeted 1
>   RSVP-TE 1
> hub-and-spoke topologies, configure with route targets 1

I

> IBGP ( internal Border Gateway Protocol)
>   defined 1
> IBGP (internal Border Gateway Protocol)
>   route reflection and 1
>   single-hop peers 1
> IGP (interior gateway protocol) 1
> IGP-LDP synchronization 1
> import map
>   setting the BGP/MPLS VPN 1
>   use 1
> import map command 1
> index command 1
> inheritance of BGP configuration values 1
> instances, L2VPN
>   configure 1
>   overview 1
> instances, VPLS
>   configuring 1, 2, 3
>   overview 1
> Integrated Local Management Interface (ILMI) cells
>   and transmission along with data cells on the same pseudowire
>     same VCI/VPI values as the data cells 1
> inter-AS (interprovider) services
>   IPv4 1
>   IPv6 1
> interface commands
>   interface loopback 1, 2
> interface tunnel command
>   MPLS 1, 2, 3
> interfaces
>   assigning to BGP sessions 1
> interior gateway protocol See IGP
> internal administrative distance, BGP 1
> internal BGP. See IBGP
> internet community, BGP 1
> intra-AS services
>   IPv4 1
>   IPv6 1
> IP addresses
>   matching route’s destination 1
> ip commands
>   ip as-path access-list 1, 2
>   ip bgp-community new-format 1
>   ip bgp-confed-as-set new-format 1
>   ip community-list 1
>   ip explicit-path command. See mpls commands, mpls explicit-path
>   ip extcommunity-list 1
>   ip prefix-list 1
>   ip prefix-tree 1
>   ip route 1, 2
>   ip route vrf 1
>   ip route-type 1
>   ip router-id 1, 2
> ip mpls commands
>   ip mpls forwarding-mode label-switched 1
> ip route parent-router command 1
> ip rsvp commands See mpls rsvp commands for all other ip rsvp commands
>   ip rsvp bandwidth.
>     mpls bandwidth See mpls commands; mpls bandwidth
> ip vrf commands
>   ip vrf 1
>   ip vrf forwarding 1, 2, 3
> IPv6 islands
>   connecting over IPv4 BGP/MPLS VPNs 1
> IPv6 VPNs
>   carrier-of-carriers 1
>   global export maps 1
>   inter-AS services 1
>   intra-AS services 1

K

> keepalive messages
>   BGP 1

L

> L-LSP 1, 2
> L2VPN address family 1, 2, 3, 4, 5, 6
> l2vpn commands
>   l2vpn control-word 1
>   l2vpn encapsulation-type 1
>   l2vpn local-site-id remote-site-id 1
>   l2vpn rd 1
>   l2vpn route-target 1
>   l2vpn sequencing 1
>   l2vpn site-name site-id 1
>   l2vpn site-range 1
> L2VPNs (Layer 2 Virtual Private Networks)
>   address families, configure 1
>   clear
>     BGP route flap dampening 1
>   configuration tasks 1
>   configure
>     address families 1
>   L2VPN address family 1, 2
>   VPWS address family 1, 2, 3
> labels, switching of MPLS 1
> layer 2 services over MPLS
>   802.3ad switch 1
>   AAL0 encapsulation 1
>   AAL5 encapsulation 1
>   ATM passthrough 1, 2
>     AAL5 encapsulation 1
>     control word support 1
>     limitations 1
>     Martini encapsulation 1
>     OAM cells 1
>     QoS classification 1
>   candidate ports 1
>   CE-side load balancing 1
>   CE-side MPLS L2VPNs over LAG
>     overview 1
>   configuration example 1
>   configuring 1
>   configuring shim interfaces 1, 2, 3
>   control word 1
>   control word support for ATM passthrough 1
>   Ethernet aggregation 1
>   Ethernet raw mode encapsulation
>     overview 1
>   Ethernet/VLAN connections 1
>   Frame Relay example 1
>   HDLC
>     configuring 1
>     overview 1
>   how they work 1
>   interfaces supported 1
>   load-balancing
>     adding member interface to group 1
>     configuring 1
>     group 1
>     monitoring 1
>     topology 1, 2
>   local cross-connects 1, 2, 3, 4
>   monitoring 1
>   MPLS L2VPN over LAG, configuration example 1
>   MPLS L2VPN over VLAN over LAG, configuration example 1
>   multiservice traffic, interface stacking for 1
>   overview 1
>   platform considerations 1
>   ports, candidate 1
>   references for 1
>   S-VLAN subinterface with an untagged C-VLAN ID
>     overview 1
>   VCC cell relay encapsulation, ATM
>     configuring 1
>     overview 1
> LDP (Label Discovery Protocol)
>   ATM n-to-one VCC cell transport (0x0009) pseudowire (PW) type
>     used for multiple VCs transmission 1
>   bringing up on the pseudowire
>     for mismatching VCI/VPI range configurations at the two pseudowire ends 1
> LDP (Label Distribution Protocol) 1
>   authentication, MD5 1
>   autoconfiguration 1
>   basic discovery 1
>   configuring for VPLS signaling 1
>   discovery mechanisms 1
>   extended discovery 1
>   FEC aggregation 1
>   FEC deaggregation 1
>   graceful restart 1
>   graceful restart configuration tasks 1
>   LDP-IGP synchronization 1
>   link hellos and discovery 1
>   messages 1
>   overview 1
>   peer discovery 1
>   targeted hellos and discovery 1
> LDP-based VPLS. See VPLS (virtual private LAN service)
> lenient behavior, BGP 1
> link hellos and LDP basic discovery 1
> list command 1
> liveness detection
>   RSVP-TE and BFD 1
> load balancing
>   candidate ports 1
>   group 1
> local administrative distance, BGP 1
> local cross-connects 1, 2, 3, 4
> local-pref attribute, BGP 1
> LSP preemption 1

M

> manuals
>   comments on 1
> maps
>   export 1
>   global export 1, 2
>   global import 1
>   import 1
> Martini ATM virtual circuits
>   over a single pseudowire 1
>     deployment scenario 1
>     overview 1
>     See also ATM virtual circuits
>   transmission of subset of
>     configuring cell concatenation for 1
>   transportation of cells from multiple circuits
>     over a single pseudowire 1
> Martini circuits
>   Ethernet packet distribution
>     configuration example 1
>   Ethernet raw mode encapsulation
>     configuration example 1
>   over LAG
>     configuration example 1
>   over VLAN over LAG
>     configuration example 1
>   with two pseudowires
>     between PE-facing routers 1
> Martini circuits over LAG
>   overview 1
> Martini layer 2 transport
>   Ethernet raw mode encapsulation, overview 1
>   S-VLAN Subinterface with an Untagged C-VLAN ID, overview 1
> match commands
>   match as-path 1
>   match community 1
>   match distance 1
>   match extcommunity 1
>   match ip address 1
>   match ip next-hop 1
>   match level 1
>   match metric 1
>   match metric-type 1
>   match mpls-label 1
>   match route-type 1
>   match tag 1
> maximum route limit, BGP/MPLS VPN 1
> maximum route warning threshold, BGP/MPLS VPN 1
> maximum routes command 1
> maximum-paths command 1
> member interface command 1
> meshed peers, reduce BGP 1
> messages, BGP 1
> MPLS (Multiprotocol Label Switching) 1
>   accounting resources 1
>   adjacency messages, LDP 1
>   administrative weight 1
>   admission control 1
>   announcing endpoints 1
>   attribute flags 1
>   authentication
>     RSVP-TE MD5 1
>   backup, LSP 1
>   bandwidth 1
>   baselining statistics 1
>   BGP/MPLS VPNs 1
>   bundle messages 1
>   bypass tunnels 1
>   class of service bits 1
>   configuration
>     basic 1
>     interface 1
>     interface profile 1
>     levels 1
>     tunnel 1
>     tunnel profile 1
>   configuring Ethernet/S-VLAN over 1, 2
>   connectivity, verify and troubleshoot 1
>   constraint-based routing 1
>   conventional IP routing 1
>   data mapping 1, 2
>   differentiated services, tunnel models for 1
>   discovery of directly connected peers 1
>   discovery of nondirectly connected peers 1
>   discovery, LDP 1
>   downstream node 1
>   downstream-on-demand 1
>   downstream-unsolicited 1
>   dynamic interfaces, creating 1
>   echo reply packets 1
>   echo request packets 1
>   ECMP
>     path tracing 1
>     support 1
>   egress forwarding actions 1
>   EXP bits 1
>   experimental bits 1
>   explicit null label 1
>   explicit path
>     configured 1
>     configuring dynamic 1
>     defining configured 1
>     dynamic 1
>   explicit routing 1
>   fast reroute extensions 1
>   fast reroute on SONET/SDX interfaces 1
>   features, supported 1
>   FEC 1
>   flooding frequency 1
>   flooding thresholds 1
>   forwarding equivalency class 1, 2
>   glossary 1
>   hard-state protocol 1
>   implicit null label 1
>   interface label space 1
>   L2VPNs, configure VPWS 1
>   label distribution protocols
>     BGP 1
>     LDP 1
>     RSVP-TE 1
>   label-switching router 1
>   labels 1, 2
>     explict null 1
>     implicit null 1
>     spaces 1
>     stacking 1
>     swapping 1
>   layer 2 services over 1
>   LDP. See LDP (Label Distribution Protocol)
>   local cross-connects 1, 2, 3
>   loose hop 1
>   LSP (label-switched path)
>     backup 1
>     configure for VPWS L2VPNs 1
>     configuring for VPLS 1
>     explicit path 1
>   LSR (label-switching router) 1
>   major interface statistics 1
>   message ack object 1
>   message ID object 1
>   monitoring 1
>   node 1
>   objects, RSVP-TE 1
>   ordered control 1
>   OSPF, configuring 1, 2
>   overview 1, 2
>   path options for backup 1
>   penultimate hop popping 1
>   platform considerations 1
>   platform label space 1
>   preemption 1
>   reachability, verify and troubleshoot 1
>   refresh messages 1
>   resource requirements 1
>   resources, configuring 1
>   route pinning 1
>   RSVP-TE. See RSVP-TE (Resource Reservation Protocol with traffic engineering extensions)
>   S bit 1
>   shim header 1
>   shim interfaces, configuring 1, 2, 3
>   soft-state protocol 1, 2
>   srefresh messages 1
>   stacking labels 1
>   statistics 1
>   statistics, major interface 1
>   strict hop 1
>   summary refresh messages 1
>   swapping labels 1
>   switching labels 1
>   switching vs routing 1
>   TLVs for ping 1
>   topology-driven LSPs 1
>   trace network connections 1
>   traffic engineering 1
>     for backup 1
>     tracking resources 1
>   TTL bits 1
>   TTL processing 1
>   TTL rules for expiration 1
>   tunnel endpoint
>     announcement 1
>     definition 1
>   tunnel metric for backup 1
>   tunnel models for differentiated services 1
>   ultimate hop popping 1
>   upstream node 1
>   VPI/VCI and labels 1
>   VPLS, configuring LSPs for 1
>   VPNs
>     BGP/MPLS 1
>   weight 1
>   See also layer 2 services over MPLS; LDP; RSVP-TE
> mpls commands 1
>   mpls 1, 2, 3, 4
>   mpls atm vci range 1
>   mpls atm vpi range 1
>   mpls backup-path 1
>   mpls bandwidth 1
>   mpls classifier-list 1
>   mpls create-dynamic-interfaces 1, 2
>   mpls diff-serv phb-id traffic-class 1
>   mpls disable 1
>   mpls explicit-path 1
>   mpls ip propagate-ttl 1
>   mpls l2-transport load-balancing-group 1
>   mpls lsp no-route retries 1
>   mpls lsp no-route retry-time 1
>   mpls lsp retries 1
>   mpls lsp retry-time 1
>   mpls policy 1
>   mpls policy-list 1
>   mpls reoptimize 1
>   mpls reoptimize timers frequency 1
>   mpls set-exp-bits 1, 2
>   mpls statistics label 1
>   mpls statistics next-hop 1, 2
>   mpls topology-driven-lsp 1
>   mpls traffic-class 1
>   mpls traffic-eng administrative-weight 1
>   mpls traffic-eng attribute-flags 1
>   mpls traffic-eng flooding threshold 1
>   mpls traffic-eng link-management timers periodic-flooding 1
>   mpls tunnel-model 1
>   mpls tunnels profile 1
>   mpls-relay 1, 2, 3, 4, 5, 6, 7
>   mpls-relay atm cell-packing mcpt-timers 1
>   mpls-relay atm vpi-range
>     1
>   See also show mpls commands
> MPLS L2VPN over LAG
>   configuration example 1
> MPLS L2VPN over VLAN over LAG
>   configuration example 1
> MPLS L2VPNs
>   over LAG, configuration example 1
>   over VLAN over LAG, configuration example 1
> MPLS L2VPNs over LAG
>   on CE-side, overview 1
> mpls ldp commands
>   mpls ldp 1, 2, 3, 4
>   mpls ldp advertise-labels 1
>   mpls ldp autoconfig 1, 2
>   mpls ldp deaggregate 1
>   mpls ldp disable 1
>   mpls ldp egress-label 1
>   mpls ldp graceful-restart 1
>   mpls ldp graceful-restart reconnect-time 1
>   mpls ldp graceful-restart recovery-time 1
>   mpls ldp graceful-restart timers max-recovery 1
>   mpls ldp graceful-restart timers neighbor-liveness 1
>   mpls ldp igp sync holddown 1
>   mpls ldp independent-control 1
>   mpls ldp ip-forwarding 1
>   mpls ldp link-hello disable 1
>   mpls ldp neighbor password 1
>   mpls ldp profile 1, 2
>   mpls ldp redistribute 1
>   mpls ldp session holdtime 1
>   mpls ldp session keepalive-interval 1
>   mpls ldp session retries 1
>   mpls ldp session retry-time 1
>   mpls ldp strict-security 1
>   mpls ldp sync 1
>   mpls ldp targeted-hello holdtime 1
>   mpls ldp targeted-hello interval 1
>   mpls ldp targeted-hello receive list 1
>   mpls ldp targeted-hello send list 1
> mpls ldp vpls commands
>   mpls ldp vpls neighbor 1
>   mpls ldp vpls vpls-id 1
> MPLS Martini circuits
>   adding on an ATM port
>     restriction for transmission of multiple ATM VCs 1
>   transmission of multiple ATM virtual circuits
>     between two ATM ports 1
>     over a single pseudowire 1
>   using the RSVP configuration
>     on the same ATM port 1
> mpls rsvp commands
>   mpls rsvp 1, 2
>   mpls rsvp authentication 1
>   mpls rsvp authentication key 1
>   mpls rsvp bfd-liveness-detection 1
>   mpls rsvp disable 1
>   mpls rsvp egress-router 1
>   mpls rsvp profile 1, 2, 3
>   mpls rsvp signalling hello 1
>   mpls rsvp signalling hello graceful-restart recovery-time 1
>   mpls rsvp signalling hello graceful-restart restart-time 1
>   mpls rsvp signalling node-hello 1
> mpls-relay atm cell-packing mcpt-timers command 1
> mpls-relay atm vpi-range command 1
> mpls-relay command
>   prerequisite for configuring
>     cell concatenation parameters for ATM ports 1
>     VCI/VPI range for ATM VCs transmission 1
> multicast IPv4 address family 1, 2, 3
> multicast IPv6 address family 1, 2, 3
> multiexit discriminator, BGP 1
> multihoming
>   for VPLS 1
> multiple ATM VCs transportation
>   over a single pseudowire
>     VPI/VCI ranges 1
> multiple ATM virtual circuits
>   transmission over a single pseudowire
>     ATMx port state 1
> Multiprotocol Label Switching. See MPLS (Multiprotocol Label Switching)
> multiservice layer 2 services 1

N

> neighbor commands
>   neighbor activate 1, 2, 3, 4
>   neighbor advertise-map 1
>   neighbor advertisement-interval 1
>   neighbor allow 1
>   neighbor allowas-in 1
>   neighbor as-override 1
>   neighbor bfd-liveness-detection 1
>   neighbor capability 1, 2
>   neighbor default-originate 1, 2
>   neighbor description 1
>   neighbor distribute-list 1
>   neighbor ebgp-multihop 1
>   neighbor filter-list 1
>   neighbor ibgp-singlehop 1
>   neighbor lenient 1
>   neighbor local-as 1
>   neighbor maximum-orf-entries 1
>   neighbor maximum-prefix 1, 2
>   neighbor maximum-update-size 1
>   neighbor next-hop-self 1, 2, 3, 4
>   neighbor passive 1
>   neighbor password 1
>   neighbor peer-group 1
>   neighbor peer-type 1
>   neighbor prefix-list 1, 2
>   neighbor prefix-tree 1
>   neighbor remote-as 1, 2
>   neighbor remote-as’ 1
>   neighbor remove-private-as 1
>   neighbor rib-out disable 1
>   neighbor route-map 1
>   neighbor route-reflector-client 1
>   neighbor send-community 1
>   neighbor send-label 1
>   neighbor shutdown 1
>   neighbor site-of-origin 1
>   neighbor soft-reconfiguration inbound 1
>   neighbor timers 1
>   neighbor unsuppress-map 1
>   neighbor update-source 1, 2
>   neighbor weight 1, 2
> neighbor graceful-restart commands
>   neighbor graceful-restart 1
>   neighbor graceful-restart restart-time 1
>   neighbor graceful-restart stalepaths-time 1
> neighbor routes, BGP 1
> neighbor weights (BGP), assign neighbor weights 1
> neighbors (peers), BGP
>   assigning weight to connections 1
>   distributing information in access lists 1
>   monitoring 1
> network area command 1
> network commands
>   network 1
>   network backdoor 1
> network connections, trace MPLS 1
> network prefixes, filtering 1
> next hops, check reachability for BGP/MPLS VPNs 1
> next-address command 1
> next-hop processing, BGP 1
> next-hop routers
>   setting or redistributing routes for 1, 2
> no synchronization command 1
> no-advertise community, BGP 1
> no-export community, BGP 1
> nontransit service 1
> notice icons 1
> notification message, BGP 1

O

> ORF (outbound route filtering) 1
> Origin attribute 1
> originator-ID, BGP 1
> OSPF interaction with BGP/MPLS VPNs 1
>   backdoor link 1
>   configuration 1
>   domain identifier attribute 1
>   route type attribute 1
>   routes
>     distributing between PEs 1
>     distributing from CE to PE 1
>     distributing from PE to CE 1
>   routing information, preserving 1
>   routing loops, preventing 1
>   sham link 1
> outbound route filtering capability 1
> overlapping VPN topologies, configuring with route targets 1
> overlapping VPNs, configuring with route targets 1
> overload shutdown command 1

P

> P routers 1
> parallel routes, maximum number of 1
> passive peers, BGP 1
> passthrough for ATM over MPLS
>   control word support 1
>   OAM cells 1
>   QoS classification 1
> path attribute, BGP 1
> path trigger delay command 1
> path, BGP 1
> PE routers 1
> peer groups, BGP 1
>   configuring 1
>   monitoring 1
> peer reachability
>   RSVP-TE 1
> peer type, set the BGP 1
> peers (neighbors), BGP
>   assigning weights to 1
>   distributing information in access lists 1
>   monitoring 1
>   passive 1
>   promiscuous 1
> per-hop behavior 1
>   nonstandard 1
> per-hop scheduling class 1
> performance impact
>   on routers
>     and transmission of multiple ATM VCs over single pseudowire 1
> PHB. See per-hop behavior
> ping mpls commands
>   ping mpls ip 1
>   ping mpls l2transport 1
>   ping mpls l3vpn 1
>   ping mpls rsvp tunnel 1
>   ping mpls vpls 1
> platform considerations
>   BGP 1
>   BGP/MPLS VPNs 1
>   L2VPNs 1
>   layer 2 services over MPLS 1
>   MPLS 1
>   VPLS 1
> policies
>   reconfiguring BGP 1
> policies, test BGP 1
> policies, VPLS subscriber. See subscriber policies for VPLS
> prefixes
>   BGP 1
>   filter network 1
> promiscuous peers, BGP 1
> provider core routers. See P routers
> provider edge routers. See PE routers
> PSC. See per-hop scheduling class
> pseudowire (PW) type
>   used for cell relay encapsulation of a single VC
>     versus multiple VCs 1
>   used for cell relay for a single VC
>     on an ATM subinterface 1
>   used for cell relay for multiple VCs
>     on an ATM port 1
> pseudowires
>   associating an ATM port with
>     before configuring cell concatenation 1
>     before configuring VCI/VPI ranges 1
>   configuration on both ends of the
>     matching in the VP/VCI range 1
>     not matching in the VPI/VCI range 1
>   failure detection
>     change of state on the ATMx port 1
>   multiple ATM virtual circuits
>     and emulation of connectivity between two ATM ports 1
>   transportation of multiple ATM virtual circuits
>     over a single wire 1
>   using a single wire for multiple VCs transport
>     topology example 1
> PWid FEC element TLV, for VPLS with LDP signaling 1

R

> rd command 1
> reachability
>   verify and troubleshoot MPLS 1
> reconvergence of BGP/MPLS VPN networks, fast 1
> redistribute command 1
> redistribution routes
>   disable dynamic (BGP) 1
> refresh messages, MPLS 1
> refresh-period command 1, 2
> remote-neighbor command 1
> reoptimization and backup 1
> reset BGP sessions 1
> RFC 4364—BGP/MPLS IP Virtual Private Networks (VPNs) (February 2006) 1, 2
> RFC 4816—Pseudowire Emulation Edge-to-Edge (PWE3) Asynchronous Transfer Mode (ATM) Transparent Cell Transport Service (February 2007) 1
> RIB (routing information base)
>   core non-VPN RIB 1, 2
>   core VPN RIB 1, 2
>   disabling RIBs-Out 1
> rib-out disable command 1
> route distinguisher 1
> route interface command 1, 2, 3
>   prerequisite for configuring
>     cell concatenation parameters for ATM ports 1
> route interface tunnel command
>   prerequisite for configuring
>     VCI/VPI range for ATM VCs transmission 1
> route maps, BGP 1
>   assigning neighbor weights 1
>   filtering incoming/outgoing routes 1
>   setting local preferences 1
> route reachability information, BGP/MPLS VPN 1
> route reflectors 1
> route target
>   defining BGP/MPLS VPN 1
> route targets
>   configuring VPN topologies 1
>   export list 1
>   for VPN topologies 1
>   import list 1
> route- refresh message , BGP 1
> route-map command 1
> route-refresh capabilities 1
> route-target address family 1, 2
> route-target command 1
> route-target extended community 1
> route-target filtering, advertisement rules with 1
> route-target filters 1
> route-target membership attribute 1
> router commands
>   router bgp 1, 2, 3, 4
>   router ospf 1
> routes
>   BGP 1
>   conditionally advertising BGP 1
>   processing of received routes for BGP/MPLS VPNs 1
>   redistributing into BGP 1
>   using BGP 1
> routing and forwarding instance. See VRF
> routing table
>   global BGP non-VPN 1, 2, 3
>   global BGP VPN 1, 2
> routing, BGP
>   conditional 1
>   confederation 1
>   default routes, configuring 1
>   maximum number of parallel routes 1, 2
>   monitoring routing table 1
>   path selection process 1
>   policy configuration 1
>   reduce the number of meshed peers 1
>   route flapping and flap damping 1
>   route reflectors 1
> routing, IP
>   monitoring 1
> RSVP-TE (Resource Reservation Protocol with traffic engineering extensions) 1
>   BFD liveness detection and 1
>   bypass tunnels 1
>   detecting path failures 1
>   fast reroute extensions 1
>   graceful restart 1
>     announcement of 1
>     preserving established LSP labels 1
>     recovery period 1
>     recovery time 1
>     restart time 1
>     restarting behavior 1
>   hello messages 1
>   MD5 authentication 1
>   overview 1
>   peer reachability 1
>   purging learned routes 1
>   refresh reduction 1
>   state synchronization 1, 2
> RT-MEM-NLRI attribute 1

S

> S-VLAN Subinterface with an Untagged C-VLAN ID
>   overview 1
> S-VLANs (stacked virtual local area networks)
>   configuring tunnel interfaces 1
>   interface stacking 1
>   tunnels 1
> SAR scheduler
>   scaling limitation
>     and number of ATM VCs in the VCI/VPI ranges 1
>   scaling limitations
>     and support of multiple VCs over a single pseudowire 1
> scalability considerations
>   transmission of multiple ATM VCs over a single pseudowire
>     and VCI/VPI ranges 1
> scaling limitations
>   on SAR scheduler
>     and support of multiple VCs over a single pseudowire 1
> sessions, BGP
>   assigning interface to 1
>   reset and clear 1
>   resetting and clearing 1, 2
> set commands
>   set comm-list delete 1
>   set community 1
>   set dampening 1, 2
>   set distance 1
>   set extcommunity 1
>   set ip next-hop 1
>   set level 1
>   set local-preference 1
>   set metric 1
>   set metric-type 1
>   set mpls-label 1
>   set origin 1
>   set route-type 1
>   set tag 1
>   set weight 1
> sham link for OSPF and BGP/MPLS VPNs 1
> shim interfaces
>   configuring VCI/VPI ranges
>     for transmission of multiple ATM VCs over a single pseudowire 1
> shim interfaces, MPLS 1, 2, 3
> show atm commands
>   show atm mcpt-timers 1
>   show atm subinterface 1
> show bgp ipv6 commands
>   show bgp ipv6 1
>   show bgp ipv6 advertised-routes 1
>   show bgp ipv6 aggregate-address 1
>   show bgp ipv6 community 1
>   show bgp ipv6 community-list 1
>   show bgp ipv6 dampened-paths 1
>   show bgp ipv6 filter-list 1
>   show bgp ipv6 flap-statistics 1
>   show bgp ipv6 inconsistent-as 1
>   show bgp ipv6 longer-prefixes 1
>   show bgp ipv6 neighbor routes 1
>   show bgp ipv6 neighbors dampened-routes 1
>   show bgp ipv6 neighbors paths 1
>   show bgp ipv6 neighbors received-routes 1
>   show bgp ipv6 network 1
>   show bgp ipv6 next-hops 1
>   show bgp ipv6 paths 1
>   show bgp ipv6 peer-group 1
>   show bgp ipv6 quote-regexp 1
>   show bgp ipv6 regexp 1
>   show bgp ipv6 summary 1
> show bridge commands
>   show bridge 1
>   show bridge groups 1
>   show bridge interface 1
>   show bridge interface vpls 1
>   show bridge port 1
>   show bridge table 1
> show cac commands
>   show cac 1
>   show cac interface 1
> show configuration commands
>   show configuration 1
> show ip bgp commands 1
>   show ip bgp 1
>   show ip bgp aggregate-address 1
>   show ip bgp cidr-only 1
>   show ip bgp community 1
>   show ip bgp community-list 1
>   show ip bgp dampened-paths 1
>   show ip bgp filter-list 1
>   show ip bgp flap-statistics 1
>   show ip bgp inconsistent-as 1
>   show ip bgp l2vpn 1, 2
>   show ip bgp l2vpn vpls 1, 2
>   show ip bgp longer-prefixes 1
>   show ip bgp neighbor routes 1
>   show ip bgp neighbors 1, 2
>   show ip bgp neighbors advertised-routes 1
>   show ip bgp neighbors dampened-routes 1
>   show ip bgp neighbors paths 1
>   show ip bgp neighbors received prefix-filter 1
>   show ip bgp neighbors received-routes 1
>   show ip bgp network 1
>   show ip bgp next-hops 1, 2, 3, 4
>   show ip bgp paths 1
>   show ip bgp peer-group 1
>   show ip bgp quote-regexp 1
>   show ip bgp regexp 1
>   show ip bgp summary 1
> show ip commands
>   show ip as-path-access-list 1
>   show ip community-list 1
>   show ip interface vrf 1
>   show ip protocols 1
>   show ip route vrf 1
>   show ip tunnel-route 1
>   show ip vrf 1
>   show ip vrf detail 1
>   show ip vrf interfaces 1
> show ipv6 commands
>   show ipv6 tunnel-route 1
> show l2vpn commands
>   show l2vpn connections 1
>   show l2vpn instance 1
>   show l2vpn interface 1
> show ldp commands
>   show ldp 1
>   show ldp binding 1
>   show ldp interface 1
>   show ldp neighbor 1
>   show ldp profile 1
>   show ldp statistics 1
>   show ldp targeted-hello 1
>   show ldp vpls 1
> show mpls commands
>   show mpls 1, 2, 3
>   show mpls binding 1
>   show mpls cross-connects atm 1
>   show mpls explicit-paths 1
>   show mpls fast-reroute database 1
>   show mpls forwarding 1, 2, 3, 4
>   show mpls interface 1
>   show mpls interface shim 1
>     verifying cell concatenation configuration for multiple ATM VCs transport 1
>     verifying VCI/VPI range specificationn for multiple ATM VCs transport 1
>   show mpls l2-transport load-balancing-group 1
>   show mpls l2transport interface 1, 2
>     verifying cell concatenation configuration for multiple ATM VCs transport 1
>     verifying VCI/VPI range for multiple ATM VCs transport 1
>   show mpls next-hop 1
>   show mpls phb-id 1
>   show mpls profile 1
>   show mpls rsvp 1
>   show mpls rsvp authentication 1
>   show mpls rsvp bfd interfaces 1
>   show mpls rsvp counters 1
>   show mpls rsvp hello graceful restart 1
>   show mpls rsvp hello instance 1
>   show mpls rsvp profile.
>     show mpls profile See show mpls commands show mpls profile
>   show mpls tunnels 1, 2
>   show mpls tunnels profile.
>     show mpls profile See show mpls commands show mpls profile
> show mpls ldp commands See show ldp commands
>   show mpls ldp igp-sync 1
> show subscriber-policy command 1
> show vpls connections command 1
> signaling, VPLS
>   BGP overview 1
>   LDP overview 1
> single-hop IBGP peers 1
> soft clear of BGP sessions 1
> speakers, BGP 1
>   route reflection and 1
> srefresh messages 1
> subscriber policies for VPLS 1
> subset of ATM virtual circuits
>   transportation over a single pseudowire
>     configuring and 1
> summary refresh messages, MPLS 1
> summary-only keyword (aggregate-address) 1
> support, technical See technical support
> switch, 802.3ad 1
> synchronization
>   enabling BGP 1
>   LDP-IGP 1
> synchronization command 1

T

> table-map command
>   BGP 1
> targeted hellos and LDP extended discovery 1
> targeted sessions, for VPLS with LDP signaling 1
> technical support
>   contacting JTAC 1
> test bgp ipv6 command 1
> test ip bgp neighbor command 1, 2
> text and syntax conventions 1
> timers bgp command 1
> topology-driven LSPs, MPLS 1
> trace mpls commands
>   trace mpls ip 1
>   trace mpls l2transport 1
>   trace mpls l3vpn 1
>   trace mpls rsvp tunnel 1
>   trace mpls vpls 1
> transit service 1
> transparent bridging and VPLS 1
> transport virtual router, configure for VPLS 1
> transportation of multiple ATM VCs
>   over a single pseudowire
>     and VPI/VCI ranges 1
> trigger delay 1
> troubleshooting
>   BGP 1
> ttl command 1
> TTL processing, MPLS
>   expiration rules 1
>   in the platform label space 1
> tunnel commands
>   tunnel destination 1, 2
> tunnel mpls commands
>   tunnel mpls affinity 1, 2
>   tunnel mpls autoroute announce 1, 2
>   tunnel mpls autoroute metric 1, 2
>   tunnel mpls bandwidth 1, 2
>   tunnel mpls description 1, 2
>   tunnel mpls diff-serv phb-id 1
>   tunnel mpls fast-rerout 1
>   tunnel mpls lsp retries 1, 2
>   tunnel mpls lsp retry-time 1, 2
>   tunnel mpls no-route retries 1, 2
>   tunnel mpls no-route retry-time 1, 2
>   tunnel mpls path-option 1, 2, 3, 4
>   tunnel mpls priority 1, 2
> tunnels
>   IPv6 over IPv4 BGP/MPLS VPNs 1

U

> unicast hop popping, MPLs 1
> unicast IPv4 address family 1, 2, 3
> unicast IPv6 address family 1, 2, 3
> update-source command 1, 2
> updates, BGP
>   AS-path filters for 1
>   in indirectly connected networks 1
>   message explanation 1
>   minimum interval between sending 1

V

> VCC (virtual channel connection) cell relay encapsulation, ATM
>   configuring 1
>   overview 1
> VCI/VPI ranges
>   configuration dependent on
>     associating the ATM port with the pseudowire 1
>   configuration for multiple VCs transmission
>     activated, deactivated 1
>   requirements for configuration of
>     for multiple ATM VCs transportation 1
> VEs (VPLS edge devices) 1
> virtual channel connection. See VCC cell relay encapsulation
> virtual private LAN service. See VPLS (virtual private LAN service)
> Virtual Private Wire Service. See VPWS (virtual private wire service L2VPNs)
> virtual-router command 1
> VPI/VCI ranges
>   configuring for multiple VCs transport
>     guidelines to be followed 1
>   configuring using
>     the mpls-relay atm vpi-range command 1
>   matching configurations
>     on both sides of the pseudowire for multiple VCs transmission 1
>   maximum number supported
>     for multiple VCs transport over a single pseudowire 1
>   mismatching configurations
>     on both sides of the pseudowire for multiple VCs transmission 1
>   number of ATM VCs in the specified configuration
>     and scaling limit of the SAR device 1
> VPLS (virtual private LAN service)
>   BGP-based
>     address families, configuring 1
>     BGP signaling, configuring 1, 2
>     BGP/MPLS VPNs 1
>     configuration example 1
>     configuration tasks for BGP signaling 1
>     L2VPN address family 1, 2
>     loopback interface and router ID, configuring 1
>     monitoring BGP-related settings 1
>     sample topology, configuring 1
>     signaling overview 1
>     VPLS address family 1, 2
>     VPLS instances for BGP signaling, configuring 1
>   CEs (customer edge devices) 1
>   clear
>     BGP attributes 1
>     BGP reachability 1
>     BGP route flap dampening 1
>     BGP wait for end-of-RIB marker 1
>     forwarding tables 1
>     LDP attributes 1
>   configure
>     MPLS LSPs 1
>     subscriber policies 1
>     VPLS instances 1
>     VPLS network interfaces 1
>   features supported 1
>   forwarding tables
>     clearing 1
>     overview 1
>   instances
>     overview 1
>   LDP-based
>     configuration example 1
>     configuration tasks for LDP signaling 1
>     LDP signaling, configuring 1, 2
>     loopback interface and router ID, configuring 1
>     monitoring LDP-related settings 1
>     sample topology, configuring 1
>     signaling overview 1
>     VPLS instances for LDP signaling, configuring 1
>   module support 1
>   monitor
>     bridging-related settings 1
>     MPLS-related settings 1
>     statistics baselines 1
>     VPLS-specific settings 1
>   multihoming 1
>   network interfaces
>     configuring 1
>     module support 1
>     overview 1
>     subscriber policies 1
>   platform considerations 1
>   prerequisites 1
>   references 1
>   subscriber policies on 1
>   transparent bridging, comparison to 1
>   transport virtual router, configure 1
>   VEs (VPLS edge devices) 1
>   virtual core interfaces
>     module support 1
>     overview 1
>   VPLS domains 1
> VPLS address family 1, 2, 3, 4, 5
> VPLS edge devices. See VEs
> VPN-IPv4
>   address 1
>   exchanging addresses 1
> VPN-IPv4 address family 1, 2, 3
> VPN-IPv6 address family 1, 2, 3
> VPNs (virtual private networks
>   BGP/MPLS hub-and-spoke example 1
> VPNs (virtual private networks)
>   BGP/MPLS 1
>   BGP/MPLS fully meshed example 1
>   carrier-of-carriers 1
>   carrier-of-carriers IPv4 1
>   configuring VPN topologies with route targets 1
>   default route to shared interface 1
>   ECMP 1
>   fallback global 1
>     example 1
>   full-mesh VPN topologies, configure with route targets 1
>   hierarchical 1
>   providing Internet access 1
>   secondary routing table lookup 1
>   static routes to shared IP interface 1
>   traffic flow from Internet to VPN 1
>   traffic flow from VPN to Internet 1
> VPWS (virtual private wire service L2VPNs)
>   address families, configure 1
>   BGP signaling, configuring 1
>   BGP/MPLS VPNs 1
>   CE (customer edge device) 1
>   clear
>     BGP reachability 1
>     BGP route flap dampening 1
>     BGP wait for end-of-RIB marker 1
>   components 1
>   configuration example 1
>   configure
>     address families 1
>     BGP signaling 1
>     L2VPN instances 1
>     L2VPN interfaces 1
>     MPLS LSPs 1
>     sample topology 1
>   features supported 1
>   instances
>     configure 1
>     overview 1
>   interfaces
>     configure 1
>   L2VPN address family 1
>   module support 1
>   monitor
>     BGP-related settings 1
>     L2VPN-specific settings 1
>     MPLS-related settings 1
>   MPLS, configure 1
>   network interfaces
>     overview 1
>   overview 1
>   PE (provider edge router) 1
>   platform considerations 1
>   prerequisites 1
>   references 1
>   VPWS address family 1, 2
> VPWS address family 1, 2, 3, 4, 5, 6
> VRF (VPN routing and forwarding instance) 1
>   carrier-of-carriers 1
>   exporting imported routes 1
>   exporting routes to global BGP non-VPN routing table 1
>   importing routes 1, 2
>   routes, exporting and importing 1

W

> weights, BGP neighbor 1
>   assign with neighbor weight command 1
>   assigning with access list 1
>   assigning with filter list 1
>   assigning with route maps 1

[Contents] [Prev] [Next] [Index] [Report an Error]