> - Downloads
> - slot ignore-diagnostic-failure

> # slot ignore-diagnostic-failure

> #### Syntax

> [ no ] slot ignore-diagnostic-failure slotNum

> #### Release Information

> Command introduced in JUNOSe Release 9.3.0.

> #### Description

> Enables you to ignore diagnostics test failures on the line module or SRP. The no version returns you to the default allowing diagnostic test failures to occur.

> #### Options

> - slotNum—Number of the selected slot in the router; for ERX7xx models, a number in the range 0–6; for ERX14xx models, a number in the range 0–13; for the ERX310 router, a number in the range 1–2; for the E120 router, a number in the range 0–5; for the E320 router, a number in the range 0–16

> #### Mode

> Global Configuration

> #### Published: 2009-10-09

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.