> - Downloads
> - controlled-interface-type
> - Related Topics
> - Configuring a Basic Parameter Definition for QoS Administrators
> - Creating a QoS Parameter on an Interface Superset or Interface Set

> # controlled-interface-type

> #### Syntax

> controlled-interface-type { controlledInterfaceType | set | superset }

> no controlled-interface-type { controlledInterfaceType | all }

> #### Release Information

> Command introduced in JUNOSe Release 7.1.0.

> set and superset keywords added in JUNOSe Release 9.2.0.

> #### Description

> Assigns controlled-interface types to a QoS parameter definition. Controlled-interface types specify the types of logical interfaces whose queues and nodes can be controlled by instances of the parameter definition. You can specify up to four controlled-interface types for each parameter definition. The no version removes the controlled-interface type from the parameter definition.

> #### Options

> - controlledInterfaceType—One of the following controlled-interface types: atm, atm-vc, atm-vp, bridge, ethernet, fr-vc, ip, ip-tunnel, ipv6, l2tp-session, l2tp-tunnel, lsp, serial, svlan, server-port, vlan
> - set—Specifies an interface set as a controlled-interface type
> - superset—Specifies an interface superset as a controlled-interface type
> - all—Removes all controlled-interface types

> #### Mode

> QoS Parameter Definition

> #### Published: 2009-10-09

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.