> - Downloads
> - next-interface
> - Related Topics
> - Policy Rule Precedence

> # next-interface

> #### Syntax

> [ no ] [ suspend ] next-interface interfaceType interfaceSpecifier
> [ next-hop nextHop ] [ classifier-group claclName ] [ precedence precValue ]

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Defines an output interface for an IP policy list. When the interfaceType is a broadcast medium, specify a next hop using the next-hop command. The no version removes a next interface rule from a policy list; the suspend keyword temporarily suspends the rule; the no suspend version resumes application of a suspended rule. For IP interfaces, this command is supported only on input policies.

> | Note: The next-interface command has been replaced by the forward interface command and may be removed completely in a future release. The SRP module Fast Ethernet port cannot be the destination of the next-interface command.

> #### Options

> - interfaceType—Interface type; see Interface Types and Specifiers
> - interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
> - nextHop—Next-hop IP address
> - claclName—In Policy List Configuration, specifies the classifier control list used to classify packets for this next-hop policy. If you do not specify a classifier group, the router selects all packets from the interface associated with this policy list for this rule.
> - precValue—In Policy List Configuration, specifies the precedence of this rule in relation to other rules within this set

> #### Mode

> Classifier Group Configuration, Policy List Configuration

> #### Published: 2009-10-08

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.