[Contents] [Prev] [Next] [Index] [Report an Error]

## pimAutoRPRcvdLog

#### Description

Protocol Independent Multicast (PIM) AutoRP messages received

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

None

#### Warning Log

None

#### Notice Log

None

#### Info

Short description of received PIM AutoRP packets

#### Debug

Complete print of received PIM AutoRP packets

#### Filter 1

interface-ip-address [ ip-address ipAddress | unnumbered interfaceType interfaceSpecifier ]

- interface-ip-address—Logs events for a specific interface
- ip-address—Specifies that you will identify the interface by entering an IP address
- ipAddress—IP address of interface for which you want to log events
- unnumbered—Specifies that the interface is unnumbered
- interfaceType—Type of interface for which you want to log events
- interfaceSpecifier—Location of unnumbered interface in the appropriate format

  | Note: For information about interface types and specifiers, see Interface Types and Specifiers in JUNOSe Command Reference Guide.

#### Filter 2

router virtualRouterName [ interface-ip-address [ ip-address ipAddress | unnumbered interfaceType interfaceSpecifier ] ]

- router—Logs events for a specific virtual router
- virtualRouterName—Name of virtual router for which you want to log events
- interface-ip-address—Logs events for a specific interface on the virtual router
- ip-address—Specifies that you will identify the interface by entering an IP address
- ipAddress—IP address of interface for which you want to log events
- unnumbered—Specifies that the interface is unnumbered
- interfaceType—Type of interface for which you want to log events
- interfaceSpecifier—Location of unnumbered interface in the appropriate format

  | Note: For information about interface types and specifiers, see Interface Types and Specifiers in JUNOSe Command Reference Guide.

[Contents] [Prev] [Next] [Index] [Report an Error]