> - Downloads
> - member-interface-type
> - Related Topics
> - Configuring Interface Sets for QoS

> # member-interface-type

> #### Syntax

> member-interface-type {vlan | atm-vc | ip}

> no member-interface-type

> #### Release Information

> Command introduced in JUNOSe Release 9.2.0.

> #### Description

> Configures the member-interface type for a QoS interface set. The no version removes the member-interface type from the parameter definition.

> #### Options

> - vlan—Specifies the member-interface-type as VLAN
> - atm–vc—Specifies the member-interface-type as VLAN
> - ip—Specifies the member-interface-type as VLAN

> #### Mode

> QoS Interface Set Configuration

> #### Published: 2009-10-09

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.