> - Downloads
> - link failover arp-flush

> # link failover arp-flush

> #### Syntax

> [ no ] link failover arp-flush

> #### Release Information

> Command introduced in JUNOSe Release 10.3.0.

> #### Description

> Clears the ARP cache on an interface with redundant ports when the primary link fails. The no version maintains the ARP entries on the interface.

> #### Mode

> Interface Configuration

> #### Published: 2009-10-09

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.