[Contents] [Prev] [Next] [Index] [Report an Error]

## Index

Symbols A B C D E F G H I L M N O P Q R S T V W Z

Symbols

> 10-Gigabit Ethernet
>   monitoring 1
> 10-Gigabit Ethernet forwarding ASIC (TFA) 1, 2, 3, 4
> 802.3ad link aggregation
>   configuring for QoS 1
>   link redundancy and QoS 1

A

> aaa qos downstream-rate command 1
> Access Node Control Protocol. See ANCP
> ADSL traffic
>   managing cell tax 1
> ANCP (Access Node Control Protocol)
>   shaping downstream rates from 1, 2
> ASIC scheduler 1
> assured rate 1
> assured-rate command 1
> ATM (Asynchronous Transfer Mode)
>   cell shaping 1
>   configuration guidelines for QoS 1
>   configuring for QoS 1
>   configuring the integrated scheduler 1
>   frame shaping 1
>   monitoring 1
>   monitoring for QoS 1
>   SAR shaping 1
>   shaping for QoS 1
> atm commands
>   atm vp-tunnel 1, 2
>   atm-vp qos-parameter 1
>   atm-vp qos-profile 1
> ATM modules with relative strict priority 1
>   minimizing latency on the SAR 1
>   oversubscribing 1
> ATM SAR shaping, QoS 1
> ATM VP
>   interface attachments 1
> audience for QoS 1

B

> backpressure 1, 2
>   default integrated mode 1
>   low-cdv mode 1
>   low-latency mode 1
> best effort 1, 2
> best-effort queue 1
> best-effort scheduler node 1
> buffer-weight command 1
> burst size, setting in a shaping rate 1
> byte adjustment application
>   configuration example 1
> byte adjustment applications
>   overview 1

C

> CDV (cell delay variation) 1
> CDVT (cell delay variation tolerance) 1, 2
> cell byte-adjustment application
>   configuring 1
> cell delay variation tolerance. See CDVT
> cell delay variation. See CDV
> clear egress-queue command 1
> clear fabric-queue command 1
> clearing statistics 1
> color-based thresholds 1
> committed drop threshold 1
> committed-drop-threshold command 1
> committed-length command 1
> committed-threshold command 1, 2
> compound shared shaping. See shared shaping
> configuration examples
>   Diffserv 1
>   QoS parameters 1, 2, 3
>   QoS profiles 1
> configuring. See specific feature, product, or protocol
> conformed drop threshold 1
> conformed-drop-threshold command 1
> conformed-fraction command 1
> conformed-length command 1
> conformed-threshold command 1, 2
> constituents, shared-shaping 1
> controlled-interface-type command 1
> controlling subscriber bandwidth
>   configuration example 1, 2
> conventions
>   notice icons 1
>   text and syntax 1
> convergence-factor command 1
> customer support 1
>   contacting JTAC 1

D

> DiffServ
>   configuration example 1
>   networks 1
> documentation set
>   comments on 1
> drop profile 1
>   configuration examples for RED 1, 2, 3
>   configuration examples for WRED 1
>   configuring RED 1
>   configuring WRED 1
>   RED (random early detection) 1
> dynamic shaping of traffic 1

E

> effective weight 1
> egress forwarding ASIC (EFA) 1, 2
> Ethernet
>   802.3ad link aggregation and QoS 1
>   configuring for QoS 1, 2
>   overview for QoS 1
>   QoS shaping mode 1
> Ethernet link aggregation commands
>   member-interface 1
> event statistics 1
> exceeded drop threshold 1
> exceeded-drop-threshold command 1
> exceeded-fraction command 1
> exceeded-length command 1
> exceeded-threshold command 1, 2
> expressions 1, 2

F

> fabric-strict-priority command 1
> fabric-weight command 1
> Fast Ethernet
>   monitoring 1
> forwarding classes. See traffic classes
> forwarding rate threshold 1
> forwarding-rate-threshold command 1
> frame byte adjustment application
>   configuring 1
> frame forwarding ASIC (FFA) 1, 2

G

> Gigabit Ethernet
>   monitoring 1, 2
> group command 1, 2
> group node 1

H

> HAR (hierarchical assured rate) 1
> hierarchical assured rate. See HAR
> hierarchical round-robin. See HRR
> hierarchy, QoS scheduler 1, 2
> HRR (hierarchical round-robin) 1, 2
> HRR scheduler 1, 2
>   relative strict priority on 1, 2

I

> implicit constituents
>   selection for compound shared shaping 1
>   selection for simple shared shaping 1
> instance-interface-type command 1
> integrated scheduler
>   configuring for QoS 1
> interface profile
>   attachments 1
> IP multicast bandwidth adjustment
>   configuration example 1
>   configuring 1
>   overview 1

L

> L2TP (Layer 2 Tunneling Protocol)
>   calculating the transmit connect speed 1
>   configuring for QoS 1
>   monitoring for QoS 1
>   overview for QoS 1
> L2TP sessions
>   QoS 1
> latency 1
> layer 2 control. See ANCP
> load balancing
>   configuring parameters 1
>   hashed
>     configuring 1
>     overview 1, 2
>   munged QoS profiles 1
>   subscriber
>     configuring 1
>     enabling default configuration 1
>     overview 1, 2
> load-rebalance command 1, 2

M

> manuals
>   comments on 1
> maximum-voql command 1
> minimum-dynamic-rate-percent command 1
> monitoring. See specific feature, product, or protocol
> multiple traffic-class groups 1
> munged QoS profile
>   attachments 1
>   Ethernet link aggregation 1

N

> node command 1, 2, 3, 4, 5, 6, 7, 8
> nodes
>   best-effort scheduler 1
>   group 1
>   scheduler 1
>   system resources 1
> notice icons 1

O

> operational QoS shaping mode 1

P

> packet fragmentation, managing 1
> parameters 1, 2, 3, 4, 5
>   See also QoS parameters
> phantom nodes 1
> port shaping 1
> port-type profile, QoS 1
>   attachments 1
> profile
>   drop 1
>   QoS
>     attachment 1
>     overview 1
>     port-type 1
>   scheduler 1
>   statistics 1
> profiles 1

Q

> QoS (quality of service)
>   administrators of 1, 2
>   clients of 1, 2
>   description of 1
>   differentiated services
>     assured forwarding 1
>     expedited forwarding 1
>   extends Diffserv 1
>   features 1
>   overview 1
>   parameters 1
>   terms 1
> QoS cell mode application
>   configuration example 1
>   configuring 1
>   overview 1
> QoS commands
>   qos-mode-port 1
>   qos-parameter 1, 2
>   qos-parameter-define 1
>   qos-port-type-profile 1, 2
>   qos-profile 1, 2, 3, 4, 5, 6, 7, 8, 9, 10
>   qos-shaping-mode 1, 2, 3
>   qos-shared-shaper-control command 1
> QoS downstream rate application
>   configuring 1
>   overview 1
>   relationship with QoS cell mode 1
> QoS interface sets
>   terms 1
> QoS parameters
>   802.3ad link aggregation 1
>   audience 1
>   configuration examples 1, 2, 3
>   configuring for QoS administrators 1
>   configuring for QoS clients 1
>   overview 1
>   parameter definitions
>     assured rate 1, 2
>     cell byte adjustment 1, 2
>     configuring 1
>     expressions 1, 2, 3
>     frame byte adjustment 1, 2
>     IP multicast bandwidth adjustment 1, 2
>     overview 1
>     QoS cell mode 1, 2
>     QoS downstream rate 1, 2
>     referencing scheduler profiles 1
>     shaping rate 1, 2
>     shared-shaping rate 1, 2
>   parameter instances
>     configuring for an interface 1
>     configuring for QoS clients 1
>     configuring globally 1
>     overview 1
>   relationship with other profiles 1
>   terminology 1
>   using with Service Manager 1, 2
> QoS profile
>   ATM VP attachments 1
>   attaching 1
>   configuring 1
>   interface attachments 1
>   monitoring 1
>   munged 1, 2
>   munged attachments 1
>   overview 1
>   port-type attachments 1
>   rules illustrated 1
>   S-VLAN attachments 1
>   using with Service Manager 1
> QoS shaping mode
>   configuring 1, 2
>   overview 1
> qos-profile command 1
> queue bandwidth 1
> queue buffers 1, 2
> queue command 1, 2, 3, 4, 5, 6, 7
> queue length 1, 2
> queue profiles 1
>   color-based thresholds 1
>   configuring 1
>   monitoring 1
>   overview 1
> queue-profile command 1
> queues 1
>   system resources 1

R

> random early detection. See RED
> range command 1
> rate shaping 1
>   QoS 1
> rate statistics 1
> rate-period command 1, 2
> reaction-factor command 1
> RED (random early detection) 1, 2
>   and dynamic queue thresholds 1
>   configuration examples 1, 2, 3
>   configuring 1
>   configuring average queue length 1
>   configuring color blind RED 1
>   configuring colored RED 1
>   how it works 1
>   monitoring 1
> relative strict-priority scheduling
>   configuration example 1
>   configuring 1
>   on ATM modules 1
>     minimizing latency on the SAR 1
>     oversubscribing 1
>   setting burst size in shaping rate 1
>   shaping rate for nonstrict queues 1
>   tuning latency on strict-priority queues 1
>   zero-weight queues 1

S

> S-VLAN
>   interface attachments 1
> SAR (segmentation and reassembly) scheduler 1, 2
>   strict-priority on 1
> scheduler
>   hierarchy 1, 2
>   HRR 1
>   node, best-effort
>     best-effort scheduler 1
>   profile 1, 2
>     configuring 1
>   SAR 1
> scheduler hierarchy
>   monitoring 1
> scheduler map. See QoS profile
> scheduler-profile command 1, 2, 3
> scheduling
>   monitoring 1
> shadow nodes
>   configuration examples
>     different traffic-class group 1
>     same traffic-class group 1
>     VLAN and IP queues 1
>   configuring 1
>   interface types 1
>   overview 1
>   system resources 1
> shadow-node command 1
> shapeless tunnel 1, 2, 3
> shaping
>   using expressions for 1, 2
> shaping mode
>   configuring 1, 2
>   overview 1
> shaping rate
>   for nonstrict queues 1
>   setting burst size in 1
> shaping, QoS ATM 1
>   cell 1
>   frame 1
> shaping-rate command 1
> shared shaping
>   active constituents 1
>   compound 1
>     active constituents 1
>     configuration 1
>     configuration example, VC shared shaping 1
>     configuration example, VP shared shaping 1
>     configuration limitations 1
>     hardware dependency 1
>   considerations 1
>   constituents 1
>     active 1
>     comparison of explicit and implicit 1
>     inactive 1
>   explicit constituents
>     example 1
>     example of weighted 1
>     selection 1, 2
>   implicit constituents
>     example at best-effort node 1
>     example at best-effort queue 1
>     example for mixed interface types 1
>     selection 1
>     selection for compound 1
>     selection for simple 1
>   inactive constituents 1
>   individual shaping and 1
>   limiting bandwidth 1
>   low-CDV mode 1
>   on the SAR, limitations of 1
>   overview 1, 2
>   simple 1
>     active constituents 1
>     configuration 1
>     configuration example, Ethernet 1
>     configuration example, VC shared shaping 1
>     configuration example, VP shared shaping 1
>     controlling the algorithm 1
>     example, basic 1
>     example, on best-effort scheduler node 1
>   traffic starvation 1
>   types, simple versus compound 1, 2
> shared-shaping-constituent command 1
> shared-shaping-rate command 1, 2, 3
> show commands
>   show aaa qos downstream-rate 1
>   show atm interface 1
>   show drop-profile 1
>   show egress-queue events 1
>   show egress-queue rates 1
>   show fabric-queue 1
>   show interfaces gigabitEthernet 1
>   show interfaces lag members 1
>   show interfaces tenGigabitEthernet 1
>   show qos-parameter 1
>   show qos-parameter-define 1
>   show qos-port-type profile 1
>   show qos-profile 1
>   show qos-shared-shaper-control command 1
>   show queue-profile 1
>   show scheduler-profile 1
>   show statistics-profile 1
>   show traffic-class 1
>   show traffic-class-group 1
> show qos commands
>   show qos interface-hierarchy 1
>   show qos queue-thresholds 1
>   show qos scheduler-hierarchy 1
>   show qos shared-shaper 1
> simple shared shaping. See shared shaping
> statistics
>   ATM 1
> statistics profile 1
>   clearing 1
>   committed drop threshold 1
>   conformed drop threshold 1
>   event statistics 1
>   exceeded drop threshold 1
>   failover mode 1, 2
>   forwarding rate threshold 1
>   maximum 1
>   monitoring 1
>   overview 1
>   rate period 1, 2, 3
>   rate statistics 1
>   resource use 1
>   thresholds 1
> statistics-profile command 1
> strict-priority command 1
> strict-priority scheduling 1, 2
>   true versus relative 1
>   See also relative strict-priority scheduling
> subscriber-interface-type command 1
> support, technical See technical support
> svlan commands
>   svlan qos-parameter 1
>   svlan qos-profile 1

T

> TCP friendly 1
> technical support
>   contacting JTAC 1
> text and syntax conventions 1
> traffic classes
>   configuring 1
>   monitoring 1
>   multiple, configuration example 1
>   overview 1
> traffic flow 1
> traffic-class command 1, 2, 3, 4
> traffic-class groups
>   monitoring 1
>   multiple 1
>   overview 1
> traffic-class-group command 1
> triple play configurations 1, 2
> true strict priority scheduling 1

V

> variables
>   configuring for shared shaping 1
> VDSL traffic
>   managing packet fragmentation for 1

W

> weight command 1, 2
> weight, QoS 1
> weighted random early detection. See WRED
> WRED (weighted random early detection) 1, 2
>   configuration examples 1
>   configuring 1
>     different drop behavior for each queue 1
>     different treatment of colored packets 1
>   how it works 1
>   monitoring 1

Z

> zero-weight queues 1

[Contents] [Prev] [Next] [Index] [Report an Error]