[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Packet Mirroring Triggers

#### Purpose

Display CLI-based packet mirroring information about all packet mirroring triggers (active and inactive) that are configured on the router. This command and the output are visible only to authorized users—the mirror-enable command must be enabled before using this command.

#### Action

To display information about all packet mirroring triggers:

    host1# show mirror rules
    Total Mirror Rules Configured: 6
    Subscriber ID                  Subscriber ID       Secure Policy  Secure Policy List  Sessions
                                   Method              Type                               Mirrored
    ------------------             ------------------  -------------  ------------------  --------
    default: user@isp250.com       username            ip             securePolicyIp      4
    vpn: fred@isp100.com           username            ip             securePolicyVpn     0
    default: 192.168.10.1          ip address          ip             securePolicyIp      1
    vpn: 10.10.2.2                 ip address          l2tp           securePolicyVpn     0
    5551212                        calling station id  l2tp           securePolicyL2tp    1
    erx atm 2/1.2:0.42:0001048579  acct-session-id     ipv6           securePolicyIpv6    1

#### Meaning

Table 63 lists show mirror rules command output fields.

Table 63: show mirror rules Output Fields

Field Name | Field Description
--- | ---
Subscriber ID | Identification of the subscriber
Subscriber ID Method | Method used to identify the subscriber
Secure Policy Type | Type of secure policy; IP, IPv6, or L2TP
Secure Policy List | Name of secure policy list used for packet mirroring
Sessions Mirrored | Number of sessions currently being mirrored

#### Related Topics

- show mirror rules

[Contents] [Prev] [Next] [Index] [Report an Error]