[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring VPLS Configuration and Statistics for a Specific VPLS Instance

Purpose

Display configuration and statistics information for the specified VPLS instance.

Action

To display configuration information for a specified VPLS (vplsA):

    host1#show bridge vplsA

      BridgeGroup: vplsA(vpls)

            Bridge Mode:            default
            Aging Time:             300 secs
            Learning:               Enabled
            Max Learn:              Unlimited
            Link Status Snmp Traps: Disabled
            Subscriber Policy:      default Subscriber
            Port Count:             2
            Interface Count:        1
            Transport Virtual Rtr:  default
            Route Distinguisher:    1.1.1.1:10
            SiteName:               boston
            SiteId:                 1
            Multi-homed:            Yes
            Site-Priority:          45
            SiteRange:              10
            VPLS Route Targets
              Route Target: RT:100:1 (both)
              Route Target: RT:100:2 (both)
            Flood Next Hop: Index 1048577

Use the all keyword to display address table and statistics information for all network interfaces associated with the VPLS instance.

Meaning

Table 84 lists the show bridge command output fields.

Table 84: show bridge Output Fields

Field Name | Field Description
--- | ---
BridgeGroup | Name of the VPLS instance for which information is displayed
Bridge Mode | Bridging capability currently enabled; for a VPLS instance, this field always displays default
Aging Time | Length of time, in seconds, that a MAC address entry can remain in the forwarding table before expiring
Learning | Whether acquisition of dynamically learned MAC addresses is enabled or disabled
Max Learn | Maximum number of dynamic MAC addresses that the VPLS instance can learn
Link Status Snmp Traps | Whether SNMP link status processing is enabled or disabled
Subscriber Policy | Name of the subscriber policy currently in effect
Port Count | Number of ports currently configured for the VPLS instance, including network interfaces and the VPLS virtual core interface
Interface Count | Number of network interfaces currently configured for the VPLS instance
Transport Virtual Rtr | Name of the transport virtual router configured for the VPLS instance
Route Distinguisher | Unique route distinguisher configured for the VPLS instance
SiteName | Site name configured for the VPLS instance
SiteId | Numerical site identifier configured for the VPLS instance
Multi-homed | Status of the site. Yes designates a multihomed site. No designates a site that is not multihomed.
Site-Priority | Priority value for the VPLS instance for the multihomed site; displayed only when the value for the Multi-homed field is Yes
SiteRange | Maximum number of sites that can participate in the VPLS domain associated with the VPLS instance
VPLS Route Targets | Extended community identifiers, also known as route targets, for each VPLS instance configured on the router
Flood Next Hop | Index of the MPLS next hop to which the router floods packets with unknown destination addresses. For more information about displaying MPLS next hops and any available next-hop statistics, see Monitoring MPLS Next Hops.

#### Related Topics

- show bridge

[Contents] [Prev] [Next] [Index] [Report an Error]