[Contents] [Prev] [Next] [Index] [Report an Error]

# show dhcp binding

#### Syntax

To display information for the specified binding ID:

show dhcp binding bindingId

To display information for DHCP client bindings on the specified subnet:

show dhcp binding [ local | external | relay-proxy ] [ subnetAddress ] [ detail ] [ filter ]

To display information for DHCP client bindings for the specified IP prefix:

show dhcp binding [ local | external | relay-proxy ] [ subnetAddress ] ip-prefix ipPrefix [ detail ] [ filter ]

To display information for DHCP client bindings for the specified interface string:

show dhcp binding [ local | external | relay-proxy ] [ subnetAddress ] interface string [ detail ] [ filter ]

To display information for DHCP client bindings without a lower-layer interface:

show dhcp binding [ local | external | relay-proxy ] [ subnetAddress ] no-interface [ detail ] [ filter ]

To display information for DHCP client bindings for the specified agent-circuit-id suboption (suboption 1) string of the DHCP relay agent information option (option 82):

show dhcp binding [ local | external | relay-proxy ] [ subnetAddress ] circuit-id string [ detail ] [ filter ]

To display information for DHCP client bindings for the specified agent-remote-id suboption (suboption 2) string of the DHCP relay agent information option (option 82):

show dhcp binding [ local | external | relay-proxy ] [ subnetAddress ] remote-id string [ detail ] [ filter ]

#### Release Information

Command introduced in JUNOSe Release 8.1.0.

local, external, relay-proxy, interface, no-interface, ip-prefix, circuit-id, and remote-id keywords and subnetAddress, ipAddress, and string variables added in JUNOSe Release 9.3.0.

#### Description

Displays information for specified DHCP client bindings, with results ordered by binding ID.

| Note: This command replaces the deprecated show ip dhcp-external binding, show ip dhcp-external binding-id, and show ip dhcp-local binding commands, which may be removed completely in a future release.

#### Options

- bindingId—DHCP binding ID for a specific client
- local—Specifies DHCP local server client bindings that meet the display criteria
- external—Specifies DHCP external server client bindings that meet the display criteria
- relay-proxy—Specifies DHCP relay proxy client bindings that meet the display criteria
- subnetAddress—IP address of the subnet on which the DHCP clients reside
- ipPrefix—IP prefix (address and subnetwork mask) of the DHCP clients; for example, 10.10.10.0/24
- no-interface—Specifies DHCP clients without a lower-layer interface; use this keyword to display information for DHCP client bindings configured over dynamic interfaces for which the lower-layer interface has been shut down
- detail—Shows detailed information for the specified DHCP bindings
- filter—See Filtering show Commands
- string—Regular expression string that represents the interface, circuit ID, or remote ID to be matched; you must enclose elements containing a space within double quotes (“one element”)

  Each element is either a literal string, a metacharacter, or a combination. You can remove the special meaning of a metacharacter by preceding it with a backslash (\). Regular expressions support the following metacharacters:

  - ^ Matches the beginning of the input string. Alternatively, when used as the first character within brackets—[^ ]—matches any number except the ones specified within the brackets.
  - $ Matches the end of the input string
  - . (period) Matches any single character, including white space
  - * Matches 0 or more sequences of the immediately previous character or pattern.
  - + Matches 1 or more sequences of the immediately previous character or pattern
  - ? Matches 0 or 1 sequence of the immediately previous character or pattern
  - ( ) Specifies patterns for multiple use when followed by one of the multiplier metacharacters: asterisk *, plus sign +, or question mark ?
  - [ ] Matches any enclosed character; specifies a range of single characters
  - – (hyphen) Used within brackets to specify a range of AS or community numbers
  - _ (underscore) Matches a ^, a $, a comma, a space, a {, or a }. Placed on either side of a string to specify a literal and disallow substring matching. Numerals enclosed by underscores can be preceded or followed by any of the characters listed above
  - | Matches characters on either side of the metacharacter; logical OR

  You must specify the interface string as a regular expression without spaces; for example, fastEthernet1.1/100 or fastEthernet.*100

  The following rules apply for representing nonprintable character sequences in the circuit ID string or the remote ID string:

  - To represent the binary sequence 0d 0a (hex), use the string '\\r\\n'. This consists of four ASCII characters: 5c for \\, 72 for r, 5c for \\, and 6e for n.

    For example, to match the sequence 74 65 73 74 0d 0a 6f 6e 65 (hex), use the string 'test\\r\\none'. In this string, 74 is represented by t, 65 is represented by e, 73 is represented by s, 74 is represented by t, 0d 0a is represented by \\r\\n, 6f is represented by o, 6e is represented by n, and 65 is represented by e.

  - To represent the binary sequence 0d 00 (hex), use the string '\\r'. This consists of two ASCII characters: 5c for \\, and 72 for r.
  - To represent the binary sequence 0a 00 (hex), use the string '\\n'. This consists of two ASCII characters: 5c for \\, and 6e for n.

    For example, to match the sequence 74 65 73 74 0a 00 6f 6e 65 (hex), use the string 'test\\none'. In this string, 74 is represented by t, 65 is represented by e, 73 is represented by s, 74 is represented by t, 0a 00 is represented by \\n, 0a is represented by \\n, 6f is represented by o, 6e is represented by n, and 65 is represented by e.

  - To represent all other cases, use the string '\\xab', where ab is a hex code of the byte. For example, to represent byte 3A, use '\\x3a'. This consists of four ASCII characters: 5c for \\, 78 for x, 33 for 3, and 61 for a.

    As another example, to match the sequence 74 65 73 74 f3 6f 6e 65 (hex), use the string 'test\\xf3one'. In this string, 74 is represented by t, 65 is represented by e, 73 is represented by s, 74 is represented by t, byte F3 is represented by \\xf3, 6f is represented by o, 6e is represented by n, and 65 is represented by e.

#### Mode

Privileged Exec

#### Related Topics

- Monitoring DHCP Binding Information

[Contents] [Prev] [Next] [Index] [Report an Error]