[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring the Tunneling Model for Differentiated Services

The JUNOSe software supports both the pipe model and the uniform model for tunneling with the mpls tunnel-model command. The router also provides a way to implement the functionality of the short pipe model for IP packets.

To specify whether MPLS uses the pipe or uniform model of tunneling for differentiated services:

- Issue the mpls tunnel-model command.
  `
  host1(config)#mpls tunnel-model uniform
  `

#### Related Topics

- Tunneling Model for Differentiated Services Overview
- Configuring MPLS and Differentiated Services
- Example Differentiated Services Application and Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]