[Contents] [Prev] [Next] [Index] [Report an Error]

# ip speed

#### Syntax

[ no ] ip speed adminSpeed

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets the speed of an IP interface in bits per second. The no version restores the default value, 0 bps.

#### Options

- adminSpeed—Speed of the interface in bps in the range 1–4294967295

#### Mode

Interface Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]