> - Downloads
> - show ip bgp next-hops
> - Related Topics
> - Monitoring BGP-Related Settings for L2VPNs, Monitoring BGP Next Hops for L2VPNs, and Monitoring BGP Next Hops for VPLS in the JUNOSe BGP and MPLS Configuration Guide

> # show ip bgp next-hops

> #### Syntax

> show ip bgp [ ipv4 unicast | ipv4 multicast | vpnv4 all | vpnv4 vrf vrfName |
> l2vpn all | l2vpn vpls vplsName | l2vpn vpws vpwsName } | route-target signaling ]
> next-hops [ ipAddress ] [ filter ]

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.
> l2vpn and all keywords added in JUNOSe Release 7.1.0.
> vpls keyword and vplsName variable added in JUNOSe Release 7.1.0.
> vpws keyword and vpwsName variable added in JUNOSe Release 8.1.0.
> route-target signaling keywords added in JUNOSe Release 8.2.0.

> #### Description

> Displays information about BGP next hops.

> #### Options

> - ipv4 unicast—Specifies the IPv4 unicast address family and routing table; the default option
> - ipv4 multicast—Specifies the IPv4 multicast address family and routing table
> - vpnv4 all—Specifies the IPv4 VPN address family and all IPv4 VPN routing and forwarding instances
> - vpvn4 vrf vrfName—Specifies the IPv4 VPN address family and only the IPv4 VPN routing and forwarding instance with the name vrfName
> - l2vpn all—Specifies all VPLS and VPWS instances in the L2VPN address family
> - l2vpn vpls vplsName—Specifies the VPLS instance with the name vplsName
> - l2vpn vpws vpwsName—Specifies the VPWS instance with the name vpwsName
> - route-target signaling—Displays information for only the route-target address family
> - ipAddress—Displays information only for this indirect next hop
> - filter—See Filtering show Commands

> #### Mode

> Privileged Exec, User Exec

> #### Published: 2009-10-08

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.