[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring VRRP

You can use several VRRP show commands to display the details of your VRRP configuration.

baseline ip vrrp

- Use to establish the baseline on all VRRP statistics as the current value.
- Example
  `
  host1#baseline ip vrrp
  `
- See baseline ip vrrp.

show ip vrrp

- Use to display a detailed summary of all configured VRIDs.

- Use the interface keyword to specify a specific Fast Ethernet, Gigabit Ethernet, or 10-Gigabit Ethernet interface.
- Use the summary keyword to display a summary count on all configured VRIDs
- Field descriptions
  - Interface—Fast Ethernet, Gigabit Ethernet, or 10-Gigabit Ethernet interface specifier and VRID
  - primary address—IP address used while in master state; not necessarily an associated address
  - operational state—State of the VRRP router: master, backup, or init; when the operational state is backup, the current master router IP address is provided
  - admin state—Administrative status: enabled or disabled
  - up time—Number of seconds that the VRID has been enabled in non-init state
  - interval—VRRP advertisement interval in seconds or milliseconds
  - Learning timer mode—Mode of the VRRP router: enabled or disabled; when the mode is enabled, the router learns the VRRP advertisement interval that is useful in case of failure of the master router. If the mode is disabled, the router does not learn the VRRP advertisement interval.
  - last error status—Help text used to debug any error detected
  - priority—Priority value of VRRP router
  - admin priority—Priority of the VRRP administrative router
  - auth type—The VRRP authentication type: none or text
  - preemption—VRRP router preemption status: enabled or disabled
  - accept data—VRRP router accept data status: enabled or disabled
  - assoc address(es)—IP addresses associated with the VRID
  - track object—Name and state of the tracked object and the value by which the object priority changes following an object state change
  - ip interfaces with vrrp—Number of IP interfaces using VRRP
  - entries—Total number of entries
  - entries enabled—Number of enabled entries
  - entries with owner priority—Number of entries with an owner priority
  - entries in init state—Number of entries in an initialization state
  - entries in backup state—Number of entries in a backup state
  - entries in master state—Number of entries in a master state
  - entries performing tracking—Number of entries performing tracking functions
- Example 1

      host1#show ip vrrp
      Interface: FastEthernet3/0 vrrpVrid: 1
        primary address: 12.60.1.1
        operational state: init
        admin state: disabled
        up time: N/A
        interval: 1 second
        Learning timer mode: disabled
        last error status: no error
        priority: 100  ( admin priority: 100 )
        auth type: none
        preemption: enabled
        accept data: disabled
        assoc address(es): none
        track object:  xyz  state:  Up  decrement:  10

- Example 2

      host1#show ip vrrp summary
      ip interfaces with vrrp: 1
        entries: 10
        entries enabled: 10
        entries with owner priority: 1
        entries in init state: 0
        entries in backup state: 9
        entries in master state: 1
        entries performing tracking: 2

- See show ip vrrp.

show ip vrrp brief

- Use to display a brief summary of all configured VRIDs.

- Use the interface keyword to specify a specific Fast Ethernet, Gigabit Ethernet, or 10-Gigabit Ethernet interface.
- Field descriptions
  - Interface—Fast Ethernet, Gigabit Ethernet, or 10-Gigabit Ethernet interface specifier
  - VRID—VRRP router instance configured on this interface
  - Primary Address—IP address used while in master state; not necessarily an associated address
  - State—Operational state of VRRP router: master, backup, or init
  - Adv—Advertisement interval, in seconds
  - Pri—Priority assigned to this router
  - Admin—Administrative state of the VRID: enabled or disabled
- Example

      host1#show ip vrrp brief
      Interface                VRID  Primary Address  State   Adv  Pri  Admin
      -----------------------  ----  ---------------  ------  ---  ---  --------
      fastEthernet12/8.1.1      255  123.123.123.123    init    1  100  disabled
      gigabitEthernet12/8.1.1     1          1.1.1.1  master    1  254  enabled

- See show ip vrrp.

show ip vrrp neighbor

- Use to display neighbors currently known to the VRRP routers.
- A neighbor—a router that shares a given VRID with the VRRP router—is known to the VRRP router only when the neighbor becomes a master for an IP address and sends VRRP advertisements to that effect. If a router sharing the VRID has not yet become a master, then the local router remains unaware of this neighbor and this command does not display that neighbor.
- Use the interface keyword to specify a specific Fast Ethernet, Gigabit Ethernet, or 10-Gigabit Ethernet interface.
- Field descriptions
  - Interface—Fast Ethernet, Gigabit Ethernet, or 10-Gigabit Ethernet interface specifier and VRID of neighbors known to the VRRP router
  - time discovered—Date and time that the neighbor was detected
  - primary address—Primary IP address of neighbor
  - adv interval (sec)—VRRP advertisement interval in seconds
  - priority—Priority status of VRRP router (255 = owner)
  - auth type—VRRP authentication type: none or text
  - assoc address(es)—IP addresses associated with the VRID that are advertised by the neighbor
- Example

      host1#show ip vrrp neighbor
      Interface: fastEthernet5/0.0 vrrpVrid: 1
        time discovered: 08/09/2001 07:44
        primary address: 10.0.0.1
        adv interval (sec): 1
        priority: 255 (owner)
        auth type: none
        assoc address(es): 10.0.0.1, 100.0.0.1, 101.0.0.1

      Interface: fastEthernet5/0.1 vrrpVrid: 11
        time discovered: 08/09/2001 07:44
        primary address: 11.0.0.1
        adv interval (sec): 1
        priority: 255 (owner)
        auth type: none
        assoc address(es): 11.0.0.1, 110.0.0.1, 111.0.0.1

- See show ip vrrp neighbor.

show ip vrrp statistics

- Use to display statistics of configured VRRP routers and each individual VRID.
- Use the delta keyword with the show ip vrrp statistics command to view the baseline statistics.

- Use the interface keyword with the show ip vrrp statistics command to specify a specific Fast Ethernet, Gigabit Ethernet, or 10-Gigabit Ethernet interface.
- Field descriptions
  - checksumErrors—Total number of VRRP packets received with an invalid VRRP checksum value
  - versionErrors—Total number of VRRP packets received with an unknown or unsupported version number
  - vrIdErrors—Total number of VRRP packets received with an invalid VRID for this virtual router
  - iccErrors—Count of line module notifications that did not make it to the controller
  - txErrors—Count of advertisements that did not get sent due to resource limitations
  - rxErrors—Count of advertisements received that could not be parsed by VRRP applications
  - Interface—Fast Ethernet, Gigabit Ethernet, or 10-Gigabit Ethernet interface specifier and VRID
  - becomeMaster—Total number of times that this VRID state has transitioned to master
  - advertiseRcvd—Total number of VRRP advertisements received
  - advertiseIntervalErrors—Total number of VRRP advertisement packets received for which the advertisement interval is different from the one configured for the VRID
  - authFailures—Total number of VRRP packets received that do not pass the authentication check
  - ipTtlErrors—Total number of VRRP packets received with IP TTL (time-to-live) not equal to 255
  - priorityZeroPktsRcvd—Total number of VRRP packets received with a priority of 0
  - priorityZeroPktsSent—Total number of VRRP packets sent with a priority
    of 0
  - invalidTypePktsRcvd—Total number of VRRP packets received with an invalid value in the Type field
  - addressListErrors—Total number of VRRP packets received for which the address list does not match the locally configured list for the VRID
  - invalidAuthType—Total number of VRRP packets received with an unknown authentication type
  - authTypeMismatch—Total number of VRRP packets received with an authentication type not equal to the locally configured authentication method
  - packetLengthErrors—Total number of VRRP packets received with a packet length less than the length of the VRRP header
- Example 1—statistics per interface

      host1#show ip vrrp statistics interface fastEthernet 4/0
      Globals:
        checksumErrors: 0
        versionErrors: 0
        vrIdErrors: 1
        iccErrors: 0
        txErrors: 0
        rxErrors: 0

      Interface: fastEthernet4/0 vrrpVrid: 1
        becomeMaster: 10
        advertiseRcvd: 0
        advertiseIntervalErrors: 0
        authFailures: 0
        ipTtlErrors: 0
        priorityZeroPktsRcvd: 0
        priorityZeroPktsSent: 9
        invalidTypePktsRcvd: 0
        addressListErrors: 0
        invalidAuthType: 0
        authTypeMismatch: 0
        packetLengthErrors: 0

      Interface: fastEthernet4/0 vrrpVrid: 50
        becomeMaster: 0
        advertiseRcvd: 1000
        advertiseIntervalErrors: 0
        authFailures: 0
        ipTtlErrors: 0
        priorityZeroPktsRcvd: 0
        priorityZeroPktsSent: 0
        invalidTypePktsRcvd: 0
        addressListErrors: 0
        invalidAuthType: 0
        authTypeMismatch: 0
        packetLengthErrors: 0

- Example 2—statistics per interface and VRID

      host1#show ip vrrp statistics interface fastEthernet 4/0 1
      Interface: fastEthernet4/0 vrrpVrid: 1
        becomeMaster: 0
        advertiseRcvd: 0
        advertiseIntervalErrors: 0
        authFailures: 0
        ipTtlErrors: 0
        priorityZeroPktsRcvd: 0
        priorityZeroPktsSent: 0
        invalidTypePktsRcvd: 0
        addressListErrors: 0
        invalidAuthType: 0
        authTypeMismatch: 0
        packetLengthErrors: 0

- See show ip vrrp statistics.

show ip vrrp statistics global

- Use to display the statistics of configured VRRP routers and each individual VRID.
- Use the delta keyword with the show ip vrrp statistics global command to view the baseline statistics.
- Field descriptions
  - checksumErrors—Total number of VRRP packets received with an invalid VRRP checksum value
  - versionErrors—Total number of VRRP packets received with an unknown or unsupported version number
  - vrIdErrors—Total number of VRRP packets received with an invalid VRID for this virtual router
  - iccErrors—Count of line module notifications that did not make it to the controller
  - txErrors—Count of advertisements that did not get sent due to resource limitations
  - rxErrors—Count of advertisements received that could not be parsed by VRRP applications
- Example

      host1#show ip vrrp statistics global
      Globals:
        checksumErrors: 0
        versionErrors: 0
        vrIdErrors: 0
        iccErrors: 0
        txErrors: 0
        rxErrors: 0

- See show ip vrrp statistics.

show ip vrrp summary

- Use to display a summary count on all configured VRIDs.
- Field descriptions
  - ip interfaces with vrrp—Total number of VRIDs configured on IP interfaces
  - entries—Total number of entries in all states
  - entries enabled—Number of entries that were enabled
  - entries with owner priority—Number of entries with owner priority
  - entries in init state—Number of entries in the init state
  - entries in backup state—Number of entries in the backup state
  - entries in master state—Number of entries in the master state
- Example

      host1#show ip vrrp summary
        ip interfaces with vrrp: 1
        entries: 10
        entries enabled: 10
        entries with owner priority: 1
        entries in init state: 0
        entries in backup state: 9
        entries in master state: 1

- See show ip vrrp.

show ip vrrp tracked-objects

- Use to display details of objects tracked by various VRIDs
- Field descriptions
  - Interface—Name of the interface
  - Vrid—VRRP router instance configured on the interface
  - Priority—Priority of the VRRP router
  - Object—Name of the object being tracked
  - Type—Type of object being tracked
  - State—State of the object
  - Decrement—Value by which the priority is decremented or restored following an object state change
- Example

      host1#show ip vrrp tracked-objects
      Interface           Vrid       Priority   Object        Type       State   Decrement
      ----------------    -------    --------   ------        --------   -----   ---------
      FastEthernet3/0     1          100        ERX_Bangalore IP-route   Up      12
      FastEthernet3/0     1          100        ERX_Bangalore IP-route   Up      15
      FastEthernet3/0     1          100        ERX_Bangalore IP-route   Up      10
      FastEthernet3/0     2          100        ERX_Bangalore IP-route   Up      10
      FastEthernet3/0     3          100        ERX_Bangalore IP-route   Up      12
      FastEthernet3/0     3          100        ERX_Bangalore IP-route   Up      15

- See show ip vrrp tracked-objects.

[Contents] [Prev] [Next] [Index] [Report an Error]