[Contents] [Prev] [Next] [Index] [Report an Error]

# baseline frame-relay multilinkinterface

#### Syntax

baseline frame-relay multilinkinterface interfaceType interfaceSpecifier

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets a statistics baseline for MLFR links. The router implements the baseline by reading and storing the statistics at the time the baseline is set and then subtracting this baseline whenever baseline-relative statistics are retrieved. There is no no version.

#### Options

- interfaceType—One of the following interface types listed in Interface Types and Specifiers
  - serial
  - pos
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers

#### Mode

Privileged Exec

[Contents] [Prev] [Next] [Index] [Report an Error]