[Contents] [Prev] [Next] [Index] [Report an Error]

# mpls lsp no-route retry-time

#### Syntax

mpls lsp no-route retry-time retryTime

no mpls lsp no-route retry-time

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the interval in seconds between attempts to set up an LSP for RSVP-TE after a failure due to no available route. The no version restores the default value, 5 seconds.

#### Options

- retryTime—Interval in the range 1–60

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]