[Contents] [Prev] [Next] [Index] [Report an Error]

# RADIUS-Initiated Disconnect

This section describes the RADIUS dynamic-request server’s RADIUS-initiated disconnect feature.

## Disconnect Messages

To centrally control the disconnection of remote access users, the RADIUS dynamic-request server on the router must receive and process unsolicited messages from RADIUS servers.

The RADIUS-initiated disconnect feature uses the existing format of RADIUS disconnect request and response messages. The RADIUS-initiated disconnect feature uses the following codes in its RADIUS request and response messages:

- Disconnect-Request (40)
- Disconnect-ACK (41)
- Disconnect-NAK (42)

[Contents] [Prev] [Next] [Index] [Report an Error]