[Contents] [Prev] [Next] [Index] [Report an Error]

# Performing Data Collection with the Activity Monitor (SRC CLI)

You can collect data with the Activity Monitor for specific components over a specified time. Before you perform data collection with the Activity Monitor, make sure the Activity Monitor (activity), CLI (cli), and C-Web interface (webadm) components are enabled.

To perform data collection with the Activity Monitor:

- `
  user@host> request support information
  `

To perform data collection for specific components:

- `
  user@host> request support information component
  `

  where component is one of the following:

  - acp—SRC Admission Control Plug-In
  - activity—Activity Monitor
  - agent—SNMP agent
  - appsvr—Application server
  - cli—SRC CLI
  - diameter—Diameter application
  - dsa—Dynamic Service Activator
  - extsubmon—External Subscriber Monitor
  - ims—IP multimedia subsystem
  - jdb—Juniper Networks database
  - jps—Juniper Policy Server
  - licSvr—License server
  - nic—Network information collector
  - redir—Redirect server
  - sae—SAE
  - webadm—C-Web interface

To perform data collection for a specified number of days:

- `
  user@host> request support information days
  `
  where days is in the range of 1–36500.

#### Related Topics

- Viewing Graphs (C-Web Interface)
- Viewing Graphs from a Web Page
- Monitoring Activity on C Series Controllers

[Contents] [Prev] [Next] [Index] [Report an Error]