> - Downloads
> - Configuring CMTS-Specific RKS Plug-Ins (SRC CLI)
> - Related Topics
> - Configuring CMTS-Specific RKS Plug-Ins (C-Web Interface)
> - Configuring Record-Keeping Server Peers for Plug-Ins (SRC CLI)
> - Configuring PCMM Record-Keeping Server Plug-Ins (SRC CLI)
> - Adding Objects for CMTS Devices (SRC CLI)
> - Initially Configuring the SAE

> # Configuring CMTS-Specific RKS Plug-Ins (SRC CLI)

> You can configure an RKS plug-in for specific CMTS devices. When there are events for the CMTS device, the SAE sends the events to the specified plug-in.

> Use the following configuration statement to assign a CMTS-specific RKS plug-in.

> `
> shared sae configuration driver pcmm cmts-specific-rks-plug-ins name {
>   rks-plug-in rks-plug-in ;
> }
> `

> To configure a CMTS-specific RKS plug-in:

> 1. From configuration mode, access the configuration statements for RKS plug-ins. In this sample procedure, west-region is the name of the SAE group, and cmtsPlugin is the name of the plug-in assignment.
>    `
>    user@host# edit shared sae group west-region configuration driver pcmm cmts-specific-rks-plug-ins cmtsPlugin
>    `
> 2. Specify the name of the CMTS-specific RKS plug-in.
>    `
>    [edit shared sae group west-region configuration driver pcmm cmts-specific-rks-plug-ins cmtsPlugin]
>    user@host# set rks-plug-in rks-plug-in
>    `
> 3. (Optional) Verify your configuration.

>        [edit shared sae group west-region configuration driver pcmm cmts-specific-rks-plug-ins cmtsPlugin]
>        user@host# show
>        rks-plug-in rksPlugin;

> #### Published: 2009-09-23

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.