[Contents] [Prev] [Next] [Index] [Report an Error]

## Using the NIC Resolver in Environments That Have Third-Party Devices (C-Web Interface)

If you are using the assigned IP subscriber method of logging in subscribers, and you are using the NIC to determine the subscriber’s SAE, you need to configure a resolver on the NIC. The OnePopDynamicIp sample configuration data supports this scenario. The OnePopDynamicIp configuration supports one point of presence (POP) and provides no redundancy. The realm for this configuration accommodates the situation in which IP pools are configured locally on each virtual router object.

You can access the OnePopDynamicIp configuration in the SRC CLI.

#### Related Topics

- Locating Subscriber Management Information
- Overview of Integrating Network Devices into the SRC Network
- Configuration Tasks for Integrating Third-Party Network Devices (C-Web Interface)

[Contents] [Prev] [Next] [Index] [Report an Error]