[Contents] [Prev] [Next] [Index] [Report an Error]

# Creating a Configuration

This sample procedure shows how to configure SAE properties for aggregate services as an example of how to navigate through various hierarchy levels in the CLI and use help and show commands to obtain information while working at the CLI.

In the SRC module, an aggregate service is a type of SAE service that comprises a number of individual services. Combining services lets the SRC module treat the services within an aggregate service as a unit.

The final configuration looks like this:

`

sae {
  configuration {
    aggregate-services {
      keepalive-time 172800;
      keepalive-retry-time 900;
      activation-deactivation-time 900;
      failed-notification-retry-time 92000;
    }
  }
}

`

To configure SAE properties for aggregate services:

1. Enter configuration mode.
   `
   user@host> edit
   Entering configuration mode.
   [edit]
   user@host#
   `
2. In configuration mode, move to the hierarchy level at which you configure aggregate services.
   `
   [edit]
   user@host# edit shared sae configuration aggregate-services
   [edit shared sae configuration aggregate-services]
   user@host#
   `

   Press the space bar after typing the initial characters of a word to quickly complete the word.

3. Verify which values you can set.

       [edit shared sae configuration aggregate-services]
       user@host#  set ?
       Possible completions:
         activation-deactivation-time
                              Time to activate or deactivate fragment service session (0..INF s)
         failed-notification-retry-time
                              Maximum time to send failure notifications (0..INF s)
         keepalive-retry-time Length of keepalive time period (0..INF s)
         keepalive-time       Keepalive from aggregate svce session to remote session (0..INF s)

4. Set the values for the four time intervals.
   `
   [edit shared sae configuration aggregate-services]
   user@host# set keepalive-time 172800
   user@host# set keepalive-retry-time 900
   [edit]
   user@host# set activation-deactivation-time 900
   [edit]
   user@host# set failed-notification-retry-time 9200
   `
5. Verify the configuration.

       [edit shared sae configuration aggregate-services]
       user@host# show
       keepalive-time 172800;
       keepalive-retry-time 900;
       activation-deactivation-time 900;
       failed-notification-retry-time 9200;

6. Move up one level in the hierarchy, and run the show command again.

       [edit shared sae configuration aggregate-services]
       user@host# up

       [edit shared sae configuration]
       user@host# show
       policy-management-configuration {
         enable-junose-classifier-expansion;
       }
       aggregate-services {
         keepalive-time 172800;
         keepalive-retry-time 900;
         activation-deactivation-time 900;
         failed-notification-retry-time 9200;
       }
       . . .

   The output shows the configuration for aggregate services plus any other configuration under the [shared sae configuration] hierarchy level.

7. Before you commit the configuration, verify that the configuration is correct.
   `
   [edit shared sae configuration]
   user@host# commit check
   configuration check succeeds
   `
8. Commit the configuration.
   `
   [edit shared sae configuration]
   user@host# commit
   commit complete.
   `

#### Related Topics

- Using Shortcuts to Create a Configuration
- Making Changes to the Configuration
- Initially Configuring the SAE
- Displaying the Current Configuration
- Verifying a Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]