> - Downloads
> - Configuring JUNOS Routing Platforms to Interact with the SAE
> - Related Topics
> - Specifying Router Initialization Scripts on the SAE
> - Configuring the JUNOS Routing Platform to Apply Changes It Receives from the SAE
> - Disabling Interactions Between the SAE and JUNOS Routing Platforms
> - Monitoring Interactions Between the SAE and JUNOS Routing Platforms

> # Configuring JUNOS Routing Platforms to Interact with the SAE

> To configure the JUNOS routing platform to interact with the SAE:

> 1. Include the following statements at the [edit system services service-deployment] hierarchy level.
>    `
>    [edit system services service-deployment]
>    servers server-address {
>      port port-number;
>    }
>    source-address source-address;
>    `
> 2. Use the following guidelines for the variables in these statements.
> - server-address —Specifies the IP address of the host on which you install the SAE. Be sure this setting matches the corresponding value in the SAE configuration.
> - port-number— Specifies the port number for the SAE. Be sure this setting matches the corresponding value in the SAE configuration.
> - source-address —(Optional) Specifies the IP address of the source that sends traffic to the SAE.

> #### Published: 2009-09-15

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.