> - Downloads
> - Event Traps
> - Related Topics
> - Overview of SNMP Traps
> - Configuring Event Traps
> - Alarm State Transitions

> ## Event Traps

> Table 1 lists the event traps.

> Table 1: Event Traps

> Trap Event | Trap ID | Text Displayed
> --- | --- | ---
> saeLicenseNetworkCapacity | 9 | $S:SAE:The total number of sum-weighted line cards allocated in this SRC network is $LINE_CARD_NUMBER ($THRESHOLD_PERCENTAGE)%. This $L the network ERX capacity threshold of $T sum-weighted line cards.: $A
> saeServiceSessionLicense | 11 | $S:LICENSE SERVER:$SERVICE_SESSIONS ($SERVICES_PERCENTAGE%) of the available licensed service sessions are in use.: $A
> routerConnClosed | 211 | When juniSaeRouterUseFailOver is FALSE: INFORMATION:SAE Router Driver: The router connection to $juniSaeRouterClientId has been closed.:RAISE When juniSaeRouterUseFailOver is TRUE: INFORMATION:SAE Router Driver:The router connection to $juniSaeRouterClientId has been closed and redirected to $juniSaeRouterFailOverIp:$juniSaeRouterFailOverPort:RAISE
> routerConnDown | 212 | INFORMATION:SAE Router Driver:The router connection to $juniSaeRouterClientId went down.:RAISE
> routerConnRejected | 213 | INFORMATION:SAE Router Driver:The router connection from $juniSaeRouterClientId has been rejected.:RAISE
> routerConnUp | 210 | INFORMATION:SAE Router Driver:A new router connection was established with $juniSaeRouterClientId.:RAISE
> routerConfOutOfSynch | 214 | When the trap is raised, the text displayed is: INFORMATION:SAE Router Driver: The configured state of router $juniSaeRouterClientId is out of synch with SAE. The configured action to be taken by SAE is $configuredAction.:RAISE When the trap is cleared, the text displayed is: INFORMATION:SAE Router Driver: The configured state of router $juniSaeRouterClientId is successfully resynchronized with SAE.:CLEAR
> agentStarted | 110 | INFORMATION:Agent: The agent has started.:RAISE
> agentRestartFailed | 111 | CRITICAL: Agent: The agent has failed to restart after $ATTEMPTS attempts:RAISE
> agentShutdown | 112 | INFORMATION:Agent:The agent has shutdown.:RAISE
> componentUp | 114 | INFORMATION:$I: This component is up.:RAISE
> componentDown | 115 | INFORMATION:$I: This component is down:RAISE
> dirConnected | 130 | INFORMATION:$I:The directory connection has been established with $LDAP_HOST on port $LDAP_PORT, and has a type of $CONNECTION_TYPE.:RAISE
> dirConnectionFailure | 131 | CRITICAL:$I:The directory connection with $LDAP_HOST has failed.:RAISE
> dirNotAvail | 132 | CRITICAL:$I:A directory connection is not available.:RAISE
> nicHostRedundStateSwitched | 240 | INFORMATION:NIC Host: The redundancy state of the NIC Host has switched to $juniNicHostRedundState.:RAISE
> nicHostMisconfigured | 241 | INFORMATION:NIC Host: The NIC Host failed to start due to misconfiguration. The error message is "$MESSAGE".:RAISE
> acpSyncCompleted | 290 | INFORMATION: ACP State Sync:ACP finished state sync with SAE for $juniAcpVirtualRouterName.:RAISE
> acpRedundStateSwitched | 291 | INFORMATION: ACP Host:The redundancy state of the ACP Host has switched to $juniAcpRedundState.:RAISE
> jpsAmConnUp | 260 | INFORMATION: JPS:A new application manager connection was established.:RAISE
> jpsAmConnDown | 261 | INFORMATION:JPS:The application manager connection went down.:RAISE
> jpsCmtsConnUp | 262 | INFORMATION:JPS:A new CMTS connection was established.:RAISE
> jpsCmtsConnDown | 263 | INFORMATION:JPS:A CMTS connection went down.:RAISE
> jdbReplicationFailure | 292 | When the trap is raised, the text displayed is: INFORMATION:jdbReplicationFailure:Failed to replicate LDAP data {juniSdxJdbReplicationDirection} neighbor {juniSdxJdbNeighbor}.The latest JDB replicaiton status is:{juniSdxJdbLastStatus }:RAISE When the trap is cleared, the text displayed is: INFORMATION: jdbReplicationFailure:Community directory server {juniSdxJdbNeighbor} latest update status error:CLEAR
> systemOperatingFailure | 300 | When the trap is raised, the text displayed is: INFORMATION:System:hardware failure is found with $juniSdxOperatingSensor on system $juniSdxOperatingLocation:RAISE When the trap is cleared, the text displayed is: INFORMATION:System:hardware failure with $juniSdxOperatingSensor on system $juniSdxOperatingLocation is cleared:CLEAR
> diskFailure | 301 | When the trap is raised, the text displayed is: INFORMATION:System:disk failure is found:RAISE When the trap is cleared, text displayed is: INFORMATION:System:disk failure is cleared:CLEAR

> #### Published: 2009-09-10

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.