[Contents] [Prev] [Next] [Index] [Report an Error]

# Assigning Interfaces to Congestion Points

You must assign interfaces either to VRs or to individual services under the VRs. Services inherit interface assignments from the associated VR unless you assign an interface to the individual service. This network interface lists the DNs of interfaces associated with backbone congestion points.

To assign interfaces to congestion points:

1. Click Configure>Shared>Congestion Points.
2. In the side pane, expand the desired profile.

   The Profile pane appears.

3. Enter information as described in the Help text in the main pane, and click Apply.

#### Related Topics

- Configuring Action Congestion Points
- Configuring Congestion Points for Services
- Configuring Congestion Points in the Directory

[Contents] [Prev] [Next] [Index] [Report an Error]