> - Downloads
> - Configuring Initialization Scripts
> - Related Topics
> - Configuring Initialization Scripts (C-Web Interface)
> - Specifying Application Managers for the Policy Server
> - Configuring the SAE to Interact with the JPS
> - Specifying Initialization Scripts on the SAE
> - Developing Router Initialization Scripts for JUNOSe Routers, JUNOS Routing Platforms, and Network Devices

> # Configuring Initialization Scripts

> When the SAE establishes a connection with a policy server, it runs an initialization script to customize the setup of the connection.

> Use the following configuration statement to configure the initialization script:

> `
> shared sae configuration driver scripts {
>   pcmm pcmm;
> }
> `

> To configure initialization scripts for the SAE:

> 1. From configuration mode, access the configuration statement that configures the initialization scripts.
>    `
>    user@host# edit shared sae configuration driver scripts
>    `
> 2. Specify the initialization script for a PCMM environment.
>    `
>    [edit shared sae configuration driver scripts]
>    user@host# set pcmm pcmm
>    `

>    The script is run when the connection between a policy server and the SAE is established and again when the connection is dropped. For the JPS, we recommend setting this value to amIorPublisher.

> #### Published: 2009-09-23

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.