[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Tunnel Interfaces (C-Web Interface)

A tunnel lets you use the redirect server in deployments where the JUNOSe router does not have a direct connection to the C Series Controller.

The other endpoint for the tunnel on a JUNOS or JUNOSe router must be configured for the tunnel to be operational.

To configure tunnel interfaces:

1. Click Configure, expand Interfaces, and expand the specified interface.
2. Click Tunnel.

   The Tunnel pane appears.

3. Click the Create button.
4. Enter information as described in the Help text in the main pane, and click Apply.

#### Related Topics

- Configuring Loopback Interfaces for IPv4 (C-Web Interface)
- Configuring a Static Route to Devices on Other Networks (C-Web Interface)
- Configuring Gigabit Ethernet Interfaces for IPv4 (C-Web Interface)
- Configuring Gigabit Ethernet Interfaces for IPv6 (C-Web Interface)

[Contents] [Prev] [Next] [Index] [Report an Error]