[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring NTP Authentication (C-Web Interface)

You can specify authentication keys for the various modes you configure for NTP.

To configure the authentication key for a mode:

- In the main pane, specify a key value for a mode.
  - Client mode—See Specifying a Basic NTP Configuration on a C Series Controller (C-Web Interface)
  - Server mode—See Configuring NTP Client Mode for a C Series Controller (C-Web Interface)
  - Broadcast mode—See Configuring NTP Broadcast Mode on a C Series Controller (C-Web Interface)
  - Symmetric active (peer) mode—See Configuring an NTP Peer for a C Series Controller (C-Web Interface)

#### Related Topics

- NTP Support on C Series Controllers
- Configuring NTP on a C Series Controller
- Specifying an Authentication Key for NTP on C Series Controllers (C-Web Interface)

[Contents] [Prev] [Next] [Index] [Report an Error]