> - Downloads
> - Configuring the SAE to Manage PCMM Devices (C-Web Interface)
> - Related Topics
> - For information about setting up SAE groups, see
> - Configuring the SAE to Manage PCMM Devices (SRC CLI)
> - Configuring PCMM Record-Keeping Server Plug-Ins (SRC CLI)
> - Using the SAE in a PCMM Environment

> # Configuring the SAE to Manage PCMM Devices (C-Web Interface)

> The SAE connects to the PCMM device by using a COPS over TCP connection. The PCMM device driver controls this connection.

> To configure the SAE to manage PCMM devices:

> 1. Click Configure, expand Shared>SAE>Configuration>Driver, and then click PCCM.

>    The PCCM pane appears.

> 2. Click Create, enter information as described in the Help text in the main pane, and then click Apply.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.