> - Downloads
> - Configuring an NTP Peer for a C Series Controller (C-Web Interface)
> - Related Topics
> - NTP Support on C Series Controllers
> - Configuring NTP on a C Series Controller

> # Configuring an NTP Peer for a C Series Controller (C-Web Interface)

> To configure NTP to operate as a peer:

> 1. Click Configure, expand System, and then click NTP.

>    The NTP pane appears.

> 2. In the Create new list, select Peer. Type an IPv4 or IPv6 address for the server and click OK.
> 3. Enter information as described in the Help text in the main pane, and click Apply.

>    | Note: If the remote system has authentication enabled, specify an authentication key and value. The system transmits the specified authentication key when transmitting packets.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.