> - Downloads
> - Configuring Resolution Information for a NIC Proxy (SRC CLI)
> - Related Topics
> - Before You Configure a NIC Proxy
> - Changing the Configuration for the NIC Proxy Cache (SRC CLI)
> - Configuring a NIC Proxy for NIC Replication (SRC CLI)
> - Configuration Statements for NIC Proxies
> - Overview of NIC Proxy Configuration

> # Configuring Resolution Information for a NIC Proxy (SRC CLI)

> Use the following statements to configure resolution information for a NIC proxy:

> `
> nic-proxy-configuration name resolution {
>   resolver-name resolver-name;
>   key-type key-type;
>   value-typevalue-type;
>   expect-multiple-values;
>   constraints constraints;
> }
> `

> To configure resolution information for a NIC proxy:

> 1. From configuration mode, access the configuration statement that specifies the NIC proxy configuration.
>    `
>    [edit]
>    user@host# component-hierarchy nic-proxy-configuration name resolution
>    `

>    For example:

>    `
>    [edit]
>    user@host# edit shared sae configuration nic-proxy-configuration ip resolution
>    `
> 2. Specify the NIC resolver that this NIC proxy uses.
>    `
>    [edit shared sae configuration nic-proxy-configuration ip resolution]
>    user@host# set resolver-name resolver-name
>    `

>    This resolver must be the same as one that is configured on the NIC host. For example:

>    `
>    [edit shared sae configuration nic-proxy-configuration ip resolution]
>    user@host# set resolver-name /realms/ip/A1
>    `
> 3. Specify the NIC data type that the key provides for the NIC resolution.
>    `
>    [edit shared sae configuration nic-proxy-configuration ip resolution]
>    user@host# set key-type key-type
>    `

>    For example:

>    `
>    [edit shared sae configuration nic-proxy-configuration ip resolution]
>    user@host# set key-type ip
>    `

>    To qualify data types, enter a qualifier within parentheses after the data type; for example, to specify username as a qualifier for the key LoginName:

>    `
>    [edit shared sae configuration nic-proxy-configuration ip resolution]
>    user@host# set key-type LoginName (username)
>    `
> 4. Specify the type of value to be returned in the resolution for the application that uses the NIC proxy.
>    `
>    [edit shared sae configuration nic-proxy-configuration ip resolution]
>    user@host# set value-type value-type
>    `

>    For example:

>    `
>    [edit shared sae configuration nic-proxy-configuration ip resolution]
>    user@host# set value-type SaeId
>    `
> 5. (Optional) If the key can have more than one value, specify that the key can have multiple corresponding values.
>    `
>    [edit shared sae configuration nic-proxy-configuration ip resolution]
>    user@host# set expect-multiple-values
>    `
> 6. (Optional. Available at the Advanced editing level.) If the application provides a constraint in the resolution request, specify the data type for the constraint. The constraint represents a condition that must or may be satisfied before the next stage of the resolution process can proceed.
>    `
>    [edit shared sae configuration nic-proxy-configuration ip resolution]
>    user@host# set constraints constraints
>    `

> #### Published: 2009-09-15

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.