[Contents] [Prev] [Next] [Index] [Report an Error]

# Verifying the Local Configuration for a Component

#### Purpose

Verify the local configuration for a component.

#### Action

1. From configuration mode, access the configuration statement that configures the slot connection. For example, to verify the slot configuration for the NIC:
   `
   user@host# edit slot 0 nic
   `
2. Run the show command. For example:

       [edit slot 0 nic ]
       user@host# show
       base-dn o=umc;
       java-runtime-environment ../jre/bin/java;
       java-heap-size 128m;
       snmp-agent;
       hostname DemoHost;
       initial {
         dynamic-dn "ou=dynamicConfiguration, ou=Configuration, o=Management,<base>";
         directory-connection {
           url ldap://127.0.0.1:389/;
           backup-urls ;
           principal cn=nic,ou=Components,o=Operators,<base>;
           credentials ********;
           timeout 10;
           check-interval 60;
         }
         directory-eventing {
           eventing;
           signature-dn <base>;
           polling-interval 15;
           event-base-dn <base>;
           dispatcher-pool-size 1;
         }
         static-dn "l=OnePop,l=NIC, ou=staticConfiguration, ou=Configuration, o=Management,<base>";
       }

#### Related Topics

- Configuring Basic Local Properties
- Viewing Information About Components Installed (SRC CLI)
- Local Properties for SRC Components

[Contents] [Prev] [Next] [Index] [Report an Error]