> - Downloads
> - Configuring RADIUS Authentication (C-Web Interface)
> - Related Topics
> - Configuring RADIUS Authentication (SRC CLI)
> - Configuring RADIUS and TACACS+ Authentication on a C Series Controller (C-Web Interface)
> - Configuring Authentication Order
> - Removing an Authentication Method from the Authentication Order

> # Configuring RADIUS Authentication (C-Web Interface)

> To configure information about RADIUS servers for authentication:

> 1. Click Configure>System.

>    The System pane appears.

> 2. From the Create new list, select RADIUS Server.
> 3. Type an IPv4 address or IPv6 address in the dialog box, and click OK.

>    The RADIUS Server pane appears.

> 4. Enter information as described in the Help text in the main pane, and click Apply.

> To configure a set of users that share a single account for authorization purposes, you create a template user.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.