[Contents] [Prev] [Next] [Index] [Report an Error]

# Defining a Congestion Point Profile (C-Web Interface)

You can create a congestion point profile that automatically performs congestion point classification. This profile supports only edge mode and dual mode for SRC ACP.

To define a congestion point profile:

1. Click Configure>Shared>Congestion Points.

   The Congestion Point Profile pane appears.

2. In the Create new list, select Profile. Type a name for the new profile in the dialog box, and click OK.

   The Profile screen appears.

3. Enter information as described in the Help text in the main pane, and click Apply.

#### Related Topics

- Congestion Point Expressions
- Classifying Interfaces (SRC CLI).
- Configuring Congestion Point Classification (C-Web Interface)
- Overview of Congestion Point Classification

[Contents] [Prev] [Next] [Index] [Report an Error]