> - Downloads
> - Configuring the SAE to Use TLS
> - Related Topics
> - Configuring the SAE to Use TLS
> - Configuring TLS on the SAE
> - Configuring JUNOS Routing Platforms to Interact with the SAE
> - Monitoring Interactions Between the SAE and JUNOS Routing Platforms

> # Configuring the SAE to Use TLS

> To configure the SAE to accept TLS connections, enter a port number with the set beep-server-port command in the JUNOS router driver configuration.

> See Configuring the SAE to Manage JUNOS Routing Platforms .

> #### Published: 2009-09-15

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.