[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring NTP as a Multicast Client on a C Series Controller (C-Web Interface)

To configure NTP to operate in multicast mode on a C Series Controller:

1. Click Configure, expand System>NTP, and then click Multicast Client.

   The Multicast Client pane appears.

2. Click Create, enter information as described in the Help text in the main pane, and then click Apply.

#### Related Topics

- NTP Support on C Series Controllers
- Configuring NTP on a C Series Controller

[Contents] [Prev] [Next] [Index] [Report an Error]