[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring TACACS+ Authentication (C-Web Interface)

To configure information about TACACS+ servers for authentication:

1. Click Configure, expand System, and then click Tacplus Server.

   The Tacplus Server pane appears.

2. Click Create, enter information as described in the Help text in the main pane, and then click Apply.

To configure a set of users that share a single account for authorization purposes, you create a template user.

#### Related Topics

- Configuring RADIUS and TACACS+ Authentication on a C Series Controller
- A C Series Controller as a RADIUS Client and TACACS+ Client
- Removing an SRC Authentication Method from the Authentication Order
- Example: Configuring SRC Authentication
- Configuring RADIUS Authentication (C-Web Interface)
- Configuring Authentication Order

[Contents] [Prev] [Next] [Index] [Report an Error]