[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Loopback Interfaces for IPv6 (C-Web Interface)

Loopback interfaces are for private use only by software running on the C Series Controller, to communicate with other software also running on the same C Series Controller.

To configure a loopback interface for IPv6:

1. Click Configure, and expand Interfaces>Interface: lo>Unit>Family.
2. Click Inet6.

   The Inet6 pane appears.

3. From the Create new list, select Address.
4. In the dialog box, type a name for the new address, and click OK.

#### Related Topics

- Configuring Loopback Interfaces for IPv4 (C-Web Interface)
- Configuring Gigabit Ethernet Interfaces for IPv4 (C-Web Interface)
- Configuring Gigabit Ethernet Interfaces for IPv6 (C-Web Interface)
- Configuring Tunnel Interfaces (C-Web Interface)

[Contents] [Prev] [Next] [Index] [Report an Error]