[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring RADIUS and TACACS+ Authentication on a C Series Controller (C-Web Interface)

The SRC software always performs password authentication on a C Series Controller. You can configure RADIUS and/ or TACACS+ authentication to complement password authentication. In this case, the software performs RADIUS and/or TACACS+ authentication before password authentication.

To configure RADIUS and TACACS+ authentication for users who access a C Series Controller:

1. Configure the connection to the RADIUS or TACACS+ server.

   See Configuring RADIUS Authentication (C-Web Interface).

   See Configuring TACACS+ Authentication (C-Web Interface).

2. Configure the authentication order.
3. Configure template accounts.

   See Using Remote Template Accounts and Configuring a Local User Template.

4. (Optional) Configure individual user profiles.

   See Overview of SRC User Accounts.

#### Related Topics

- Configuring RADIUS and TACACS+ Authentication on a C Series Controller
- Configuring Authentication Order
- Removing an Authentication Method from the Authentication Order

[Contents] [Prev] [Next] [Index] [Report an Error]