[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Interactions Between the SAE and JUNOS Routing Platforms

#### Purpose

Monitor the connection between the SAE and a JUNOS routing platform.

#### Action

Use the following command on JUNOS routing platforms to monitor the connection between the JUNOS routing platform and the SAE.

    root@ui1>
    show system services service-deployment

    Connected to 172.17.20.151 port 3333 since 2004-02-06 14:50:31 PST
    Keepalive settings: Interval 15 seconds
    Keepalives sent: 100, Last sent: 6 seconds ago
    Notifications sent: 0
    Last update from peer: 00:00:06 ago

You can also monitor the interactions between the SRC software and JUNOS routing platforms in the log files for the SAE and in the log files generated by the SRC software process on the JUNOS routing platform.

#### Related Topics

- Configuring JUNOS Routing Platforms to Interact with the SAE
- Configuring the JUNOS Routing Platform to Apply Changes It Receives from the SAE
- Disabling Interactions Between the SAE and JUNOS Routing Platforms
- Overview of Logging for SRC Components
- For information about configuring logging on JUNOS routing platforms, see JUNOS System Basics Configuration Guide.

[Contents] [Prev] [Next] [Index] [Report an Error]