> - Downloads
> - Configuring Classify-Traffic Conditions (C-Web Interface)
> - Related Topics
> - Before You Configure Classify-Traffic Conditions
> - Configuring Classify-Traffic Conditions
> - Enabling Expansion of JUNOSe Classify-Traffic Conditions (C-Web Interface)
> - Specifying Port Access for Traffic Classification (C-Web Interface)

> # Configuring Classify-Traffic Conditions (C-Web Interface)

> You create classify-traffic conditions in JUNOSe policy rules, in JUNOS ASP and JUNOS filter policy rules, and in PCMM policy rules.

> The available configuration statements change depending on the type of policy rule that holds the condition and on the type of protocol that you specify.

> To configure a classify-traffic condition, do the following:

> 1. Create a classify-traffic condition. See:

>    See Creating a Classify-Traffic Condition (C-Web Interface).

> 2. Configure source networks. You can configure source networks in one of two formats. See:
>    - Configuring Source Networks (C-Web Interface)
>    - Configuring Source Grouped Networks (C-Web Interface)
> 3. Configure destination networks. You can configure destination networks in one of two formats. See:
>    - Configuring Destination Networks (C-Web Interface)
>    - Configuring Destination Grouped Networks (C-Web Interface)
> 4. Configure protocol conditions. The type of protocol condition that you use depends on your configuration.
>    - To configure protocol conditions that do not include ports, see:
>      - Configuring Protocol Conditions (C-Web Interface)
>    - To configure protocol conditions that include ports, see:
>      - Configuring Protocol Conditions with Ports (C-Web Interface)
>    - To configure protocol conditions in which the protocol that you specify is a parameter, see:
>      - Configuring Protocol Conditions with Parameters (C-Web Interface)
>    - To configure protocol conditions in which the protocol is TCP, see:
>      - Configuring TCP Conditions (C-Web Interface)
>    - To configure protocol conditions in which the protocol is ICMP, see:
>      - Configuring ICMP Conditions (C-Web Interface)
>    - To configure protocol conditions in which the protocol is IGMP, see:
>      - Configuring IGMP Conditions (C-Web Interface)
>    - To configure protocol conditions in which the protocol is IPSec, see:
>      - Configuring IPSec Conditions (C-Web Interface)
>    - To configure a ToS byte condition, see:
>      - Configuring IGMP Conditions (C-Web Interface)
> 5. For JUNOS filter policies, configure a JUNOS filter condition. See:
>    - Configuring JUNOS Filter Conditions (C-Web Interface)
> 6. For the stateful firewall and NAT policies, configure an application protocol condition. See:
>    - Configuring Application Protocol Conditions (C-Web Interface)

>      | Note: PCMM classifiers support only the following classifiers: Source and destination IP addresses Network protocol Source or destination port Type-of-service (ToS) byte and ToS mask The policy engine ignores all other values.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.