[Contents] [Prev] [Next] [Index] [Report an Error]

# Verifying NTP Configuration on a C Series Controller

#### Purpose

To verify the configuration for NTP.

#### Action

At the [edit system ntp] hierarchy level, enter the show command. For example:

    [edit system ntp]
    user@host# show
    boot-server 192.0.2.20;
    multicast-client 192.0.2.15;
    trusted-key 1;
    server 192.0.2.30 key 1;
    server 192.0.2.25;
    authentication-key 1 {
      value ********;
    }

#### Related Topics

- Specifying Which NTP Server a C Series Controller Contacts on Startup
- NTP Support on C Series Controllers

[Contents] [Prev] [Next] [Index] [Report an Error]