[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Global SNMP Communities in the SRC Module (C-Web Interface)

You can configure global default SNMP communities that are used if a VR does not exist on the router or if the community strings have not been configured for the VR.

To configure global default SNMP communities:

1. Click Configure, expand Shared>SAE>Configuration>Driver, and then click SNMP.

   The SNMP pane appears.

2. Click Create, enter information as described in the Help text in the main pane, and then click Apply.

#### Related Topics

- How SNMP Obtains Information from Routers for the SRC Software

[Contents] [Prev] [Next] [Index] [Report an Error]