[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring External Subscriber Monitor (C-Web Interface)

Configure initial properties, including directory connection and directory eventing properties.

Tasks to configure External Subscriber Monitor are:

1. Configuring Basic Local Properties for External Subscriber Monitor
2. Configuring Initial Properties for External Subscriber Monitor
3. Configuring Directory Connection Properties for External Subscriber Monitor
4. Configuring Eventing Properties for External Subscriber Monitor
5. Configuring Logging Destinations for External Subscriber Monitor

## Configuring Basic Local Properties for External Subscriber Monitor

To configure basic local properties:

1. Click Configure>Slot, then a specified slot (for example, slot0), and then External Subscriber Monitor.

   The External Subscriber Monitor pane appears.

2. From the Create new list, select Logger. Type a name for the new logger in the dialog box, and click OK.
3. Enter the maximum java heap size in the Java Heap Size box, as described in the Help text.
4. Click Apply.

## Configuring Initial Properties for External Subscriber Monitor

To configure initial properties:

1. Click Configure>Slot, then a specified slot (for example, slot0).
2. Expand External Subscriber Monitor.
3. Click Initial.

   The Initial pane appears.

## Configuring Directory Connection Properties for External Subscriber Monitor

To configure directory connection properties:

1. Click Configure>Slot, then a specified slot (for example, slot0).
2. Expand External Subscriber Monitor.
3. Expand Initialand, then click Directory Connection.

   The Directory Connection pane appears.

4. Enter the information as described in the Help text box.
5. Click Apply.

## Configuring Eventing Properties for External Subscriber Monitor

To configure eventing properties:

1. Click Configure>Slot, then a specified slot (for example, slot0).
2. Expand External Subscriber Monitor.
3. Expand Initial, and then click Directory Eventing.

   The Directory Eventing pane appears.

4. Enter the information as described in the Help text box.
5. Click Apply.

## Configuring Logging Destinations for External Subscriber Monitor

You can configure the logging destination to store messages in a file or a system logging facility (Syslog). You can create or modify loggers.

To configure logging destinations to store log messages:

1. Click Configure>Slot, then a specified slot (for example, slot0).
2. Expand External Subscriber Monitor.
3. From the Create new list, select Logger.
4. In the dialog box, type a name for the new logger, and click OK.

   The name of the logger appears in the side pane and the Logger pane.

5. Expand the logger in the side pane, and then click File or Syslog.
6. Click Create, enter information as described in the Help text in the main pane, and click Apply.

[Contents] [Prev] [Next] [Index] [Report an Error]