[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Gigabit Ethernet Interfaces for IPv4 (C-Web Interface)

To allow remote access to the C Series Controller, you configure the Gigabit Ethernet interfaces. You can specify an IP address with mask or a broadcast address with mask for an interface.

To configure a Gigabit Ethernet interface for IPv4:

1. Click Configure>Interfaces.

   The Interfaces pane appears.

2. From the Create new list, create an interface.
   - To create a new interface, select Interface, type a name for the new interface in the dialog box, and click OK.
   - To create an eth1, eth2, or eth3 interface, select eth1, eth2, or eth3, and click OK.
3. To specify the unit:
   1. From the Create new list, select Unit.
   2. In the dialog box, type a number for the new unit, and click OK.
4. To specify an IPv4 address for the new unit, expand Unit: < number >, and expand Family in the side pane.
   1. In the side pane, click Inet.

      The Interfaces pane appears.

   2. Click the Create button.
   3. Enter information as described in the Help text in the main pane, and click Apply.

#### Related Topics

- Configuring Loopback Interfaces for IPv4 (C-Web Interface)
- Configuring Gigabit Ethernet Interfaces for IPv4 (C-Web Interface)
- Configuring Gigabit Ethernet Interfaces for IPv6 (C-Web Interface)
- Configuring Tunnel Interfaces (C-Web Interface)

[Contents] [Prev] [Next] [Index] [Report an Error]