[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring a NIC Proxy (C-Web Interface)

To have an application communicate with the NIC, you configure the type of resolution used by a NIC proxy.

To configure resolution information for a NIC proxy.

1. Click Configure, expand Shared>SAE, and then click Configuration.

   The Configuration pane appears.

2. From the Create new list, select NIC Proxy Configuration. Type a name for the new NIC proxy in the dialog box, and click OK.

   The new NIC proxy configuration appears in the side pane.

3. Expand the NIC proxy configuration.
4. To configure resolution information, in the side pane click Resolution.

   The Resolution pane appears.

5. Click Create, enter information as described in the Help text, and click Apply.
6. To optimize resolution performance, in the side pane click Cache.

   The Cache pane appears.

   The cache options are available at the Advanced and Expert editing levels.

7. Click Create, enter information as described in the Help text, and click Apply.
8. To keep the NIC highly available, configure NIC host selection, and define how the NIC proxy handles NIC hosts to which it cannot connect.

   The NIC Host Selection options are available at the Advanced and Expert editing levels.

   1. In the side pane, click NIC Host Selection.

      The NIC Host Selection pane appears.

   2. Click Create, enter information as described in the Help text, and then click Apply.
   3. Expand NIC Host Selection, and click Blacklisting.

      The Blacklisting pane appears.

   4. Click Create, enter information as described in the Help text, and click Apply.

#### Related Topics

- Before You Configure a NIC Proxy
- Changing NIC Configurations (SRC CLI)
- Configuring NIC Test Data (C-Web Interface)
- Examples: Key Values for NIC Bindings
- Overview of NIC Proxy Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]