> - Downloads
> - Configuring PCMM Record-Keeping Server Plug-Ins (SRC CLI)
> - Related Topics
> - Using the SAE in a PCMM Environment
> - Overview of a PCMM Environment
> - Configuring PCMM Record-Keeping Server Plug-Ins (C-Web Interface)
> - Initially Configuring the SAE

> # Configuring PCMM Record-Keeping Server Plug-Ins (SRC CLI)

> Use the following configuration statements to configure an RKS plug-in.

> `
> shared sae configuration plug-ins name name pcmm-rks {
>   load-balancing-mode (failover | roundRobin);
>   failback-timer failback-timer;
>   retry-interval retry-interval ;
>   maximum-queue-length maximum-queue-length ;
>   bind-address bind-address ;
>   udp-port udp-port ;
>   feid-mso-data feid-mso-data ;
>   feid-mso-domain-name feid-mso-domain-name ;
>   trusted-element;
>   default-peer default-peer ;
> }
> `

> To configure an RKS plug-in:

> 1. From configuration mode, access the configuration statements for RKS plug-ins. In this sample procedure, west-region is the name of the SAE group, and rksPlugin is the name of the plug-in.
>    `
>    user@host# edit shared sae group west-region configuration plug-ins name rksPlugin pcmm-rks
>    `
> 2. Specify the mode for load-balancing RKSs.
>    `
>    [edit shared sae group west-region configuration plug-ins name rksPlugin pcmm-rks]
>    user@host# set load-balancing-mode (failover | roundRobin)
>    `
> 3. Specify if and when the SAE attempts to fail back to the default peer.
>    `
>    [edit shared sae group west-region configuration plug-ins name rksPlugin pcmm-rks]
>    user@host# set failback-timer failback-timer
>    `
> 4. Specify the time the SAE waits for a response from an RKS before it resends the packet.
>    `
>    [edit shared sae group west-region configuration plug-ins name rksPlugin pcmm-rks]
>    user@host# set retry-interval retry-interval
>    `
> 5. Specify the maximum number of unacknowledged messages that the plug-in receives from the RKS before it discards new messages.
>    `
>    [edit shared sae group west-region configuration plug-ins name rksPlugin pcmm-rks]
>    user@host# set maximum-queue-length maximum-queue-length
>    `
> 6. (Optional) Specify the source IP address that the plug-in uses to communicate with the RKS.
>    `
>    [edit shared sae group west-region configuration plug-ins name rksPlugin pcmm-rks]
>    user@host# set bind-address bind-address
>    `
> 7. (Optional) Specify the source UDP port or a pool of ports that the plug-in uses to communicate with the RKS.
>    `
>    [edit shared sae group west-region configuration plug-ins name rksPlugin pcmm-rks]
>    user@host# set udp-port udp-port
>    `
> 8. (Optional) Specify the multiple service operator (MSO)—defined data in the financial entity ID (FEID) attribute, which is included in event messages.
>    `
>    [edit shared sae group west-region configuration plug-ins name rksPlugin pcmm-rks]
>    user@host# set feid-mso-data feid-mso-data
>    `
> 9. (Optional) Specify the MSO domain name in the FEID attribute that uniquely identifies the MSO for billing and settlement purposes.
>    `
>    [edit shared sae group west-region configuration plug-ins name rksPlugin pcmm-rks]
>    user@host# set feid-mso-domain-name feid-mso-domain-name
>    `
> 10. (Optional) When the SAE is running as a policy server—which means that the SAE sends event messages directly to the RKS—enable the SAE as a trusted network element.
>     `
>     [edit shared sae group west-region configuration plug-ins name rksPlugin pcmm-rks]
>     user@host# set trusted-element
>     `
> 11. Specify the name of the primary RKS peer to which the SAE sends accounting packets.

>     See Configuring Record-Keeping Server Peers for Plug-Ins (SRC CLI).

>     `
>     [edit shared sae group west-region configuration plug-ins name rksPlugin pcmm-rks]
>     user@host# set default-peer default-peer
>     `
> 12. (Optional) Verify your RKS plug-in configuration.

>         [edit shared sae group west-region configuration plug-ins name rksPlugin pcmm-rks]
>         user@host> show
>         load-balancing-mode failover;
>         failback-timer -1;
>         retry-interval 3000;
>         maximum-queue-length 10000;
>         feid-mso-domain-name abcd.com;
>         trusted-element;
>         default-peer radius01;

> 13. (Optional) Specify an RKS plug-in for specific CMTS devices.

>     See Configuring CMTS-Specific RKS Plug-Ins (SRC CLI) .

> #### Published: 2009-09-23

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.